Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## FCVTX

Floating-point down convert, rounding to odd (predicated)

Convert active double-precision floating-point elements from the source vector to single-precision, rounding to Odd, and place the results in the even-numbered 32-bit elements of the destination vector, while setting the odd-numbered elements to zero. Inactive elements in the destination vector register remain unmodified.

Rounding to Odd (aka Von Neumann rounding) permits a two-step conversion from double-precision to half-precision without incurring intermediate rounding errors.

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | 1 | 1 | 0 | 0 | 1 | 0 | 1 | 0 | 0 | 0 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 | Pg | Zn | Zd

####

FCVTX <Zd>.S, <Pg>/M, <Zn>.D

if !HaveSVE2() && !HaveSME() then UNDEFINED; constant integer esize = 64; integer g = UInt(Pg); integer n = UInt(Zn); integer d = UInt(Zd); constant integer s_esize = 64; constant integer d_esize = 32;

### Assembler Symbols

<Zd> | Is the name of the destination scalable vector register, encoded in the "Zd" field.

<Pg> | Is the name of the governing scalable predicate register P0-P7, encoded in the "Pg" field.

<Zn> | Is the name of the source scalable vector register, encoded in the "Zn" field.

### Operation

CheckSVEEnabled(); constant integer VL = CurrentVL; constant integer PL = VL DIV 8; constant integer elements = VL DIV esize; bits(PL) mask = P[g, PL]; bits(VL) operand = if AnyActiveElement(mask, esize) then Z[n, VL] else Zeros(VL); bits(VL) result = Z[d, VL]; for e = 0 to elements-1 if ActivePredicateElement(mask, e, esize) then bits(esize) element = Elem[operand, e, esize]; bits(d_esize) res = FPConvertSVE(element<s_esize-1:0>, FPCR[], FPRounding_ODD, d_esize); Elem[result, e, esize] = ZeroExtend(res, esize); Z[d, VL] = result;

### Operational information

This instruction might be immediately preceded in program order by a MOVPRFX instruction. The MOVPRFX instruction must conform to all of the following requirements, otherwise the behavior of the MOVPRFX and this instruction is unpredictable:

- The MOVPRFX instruction must be unpredicated, or be predicated using the same governing predicate register and source element size as this instruction.
- The MOVPRFX instruction must specify the same destination register as this instruction.
- The destination register must not refer to architectural register state referenced by any other source operand register of this instruction.

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: isa v33.64, AdvSIMD v29.12, pseudocode v2023-06_rel, sve v2023-06_rel ; Build timestamp: 2023-07-04T19:42

Copyright © 2010-2023 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.