Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## URSRA

Unsigned rounding shift right and accumulate (immediate)

Shift right by immediate each unsigned element of the source vector, inserting zeroes, and add the rounded intermediate result destructively to the corresponding elements of the addend vector. The immediate shift amount is an unsigned value in the range 1 to number of bits per element. This instruction is unpredicated.

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | 1 | 0 | 0 | 0 | 1 | 0 | 1 | tszh | 0 | tszl | imm3 | 1 | 1 | 1 | 0 | 1 | 1 | Zn | Zda
|  |  |  |  |  | R | U |  |

####

URSRA <Zda>.<T>, <Zn>.<T>, #<const>

if !IsFeatureImplemented(FEAT_SVE2) && !IsFeatureImplemented(FEAT_SME) then UNDEFINED; constant bits(4) tsize = tszh:tszl; if tsize == '0000' then UNDEFINED; constant integer esize = 8 << HighestSetBit(tsize); constant integer n = UInt(Zn); constant integer da = UInt(Zda); constant integer shift = (2 * esize) - UInt(tsize:imm3);

### Assembler Symbols

<Zda> | Is the name of the third source and destination scalable vector register, encoded in the "Zda" field.

<T> | Is the size specifier, encoded in tszh:tszl:
tszh | tszl | <T>
--- | --- | ---
00 | 00 | RESERVED
00 | 01 | B
00 | 1x | H
01 | xx | S
1x | xx | D

<Zn> | Is the name of the first source scalable vector register, encoded in the "Zn" field.

<const> | Is the immediate shift amount, in the range 1 to number of bits per element, encoded in "tszh:tszl:imm3".

### Operation

CheckSVEEnabled(); constant integer VL = CurrentVL; constant integer elements = VL DIV esize; constant bits(VL) operand1 = Z[n, VL]; constant bits(VL) operand2 = Z[da, VL]; bits(VL) result; for e = 0 to elements-1 constant integer element = (UInt(Elem[operand1, e, esize]) + (1 << (shift - 1))) >> shift; Elem[result, e, esize] = Elem[operand2, e, esize] + element<esize-1:0>; Z[da, VL] = result;

### Operational information

This instruction might be immediately preceded in program order by a MOVPRFX instruction. The MOVPRFX must conform to all of the following requirements, otherwise the behavior of the MOVPRFX and this instruction is constrained unpredictable:

- The MOVPRFX must be unpredicated.
- The MOVPRFX must specify the same destination register as this instruction.
- The destination register must not refer to architectural register state referenced by any other source operand register of this instruction.

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: aarchmrs v2024-03_relA, pseudocode v2024-03_rel, sve v2024-03_rel ; Build timestamp: 2024-03-26T09:45

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.