AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# PMSLATFR_EL1, Sampling Latency Filter Register

The PMSLATFR_EL1 characteristics are:

## Purpose

Controls sample filtering by latency

## Configuration

This register is present only when FEAT_SPE is implemented. Otherwise, direct accesses to PMSLATFR_EL1 are UNDEFINED.

## Attributes

PMSLATFR_EL1 is a 64-bit register.

## Field descriptions

63 | 62 | 61 | 60 | 59 | 58 | 57 | 56 | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48 | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40 | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
RES0
RES0 | MINLAT

#### Bits [63:16]

Reserved, RES0.

#### MINLAT, bits [15:0]

Minimum latency. When PMSFCR_EL1.FL is 1, defines the minimum total latency for filtered operations. Samples with a total latency less than PMSLATFR_EL1.MINLAT are not recorded.

If PMSIDR_EL1.CountSize is 0b0010, PMSLATFR_EL1.MINLAT[15:12] is RES0.

This field is ignored by the PE when PMSFCR_EL1.FL == 0.

The reset behavior of this field is:

- On a Warm reset, this field resets to an architecturally UNKNOWN value.

## Accessing PMSLATFR_EL1

Accesses to this register use the following encodings in the System register encoding space:

#### MRS <Xt>, PMSLATFR_EL1

op0 | op1 | CRn | CRm | op2
--- | --- | --- | --- | ---
0b11 | 0b000 | 0b1001 | 0b1001 | 0b110

if PSTATE.EL == EL0 then UNDEFINED; elsif PSTATE.EL == EL1 then if HaveEL(EL3) && EL3SDDUndefPriority() && (MDCR_EL3.NSPB[0] == '0' || MDCR_EL3.NSPB[1] != SCR_EL3.NS || (IsFeatureImplemented(FEAT_RME) && MDCR_EL3.NSPBE != SCR_EL3.NSE)) then UNDEFINED; elsif EL2Enabled() && IsFeatureImplemented(FEAT_FGT) && (!HaveEL(EL3) || SCR_EL3.FGTEn == '1') && HDFGRTR_EL2.PMSLATFR_EL1 == '1' then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && MDCR_EL2.TPMS == '1' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && (MDCR_EL3.NSPB[0] == '0' || MDCR_EL3.NSPB[1] != SCR_EL3.NS || (IsFeatureImplemented(FEAT_RME) && MDCR_EL3.NSPBE != SCR_EL3.NSE)) then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif EffectiveHCR_EL2_NVx() IN {'1x1'} then X[t, 64] = NVMem[0x848]; else X[t, 64] = PMSLATFR_EL1; elsif PSTATE.EL == EL2 then if HaveEL(EL3) && EL3SDDUndefPriority() && (MDCR_EL3.NSPB[0] == '0' || MDCR_EL3.NSPB[1] != SCR_EL3.NS || (IsFeatureImplemented(FEAT_RME) && MDCR_EL3.NSPBE != SCR_EL3.NSE)) then UNDEFINED; elsif HaveEL(EL3) && (MDCR_EL3.NSPB[0] == '0' || MDCR_EL3.NSPB[1] != SCR_EL3.NS || (IsFeatureImplemented(FEAT_RME) && MDCR_EL3.NSPBE != SCR_EL3.NSE)) then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); else X[t, 64] = PMSLATFR_EL1; elsif PSTATE.EL == EL3 then X[t, 64] = PMSLATFR_EL1;

#### MSR PMSLATFR_EL1, <Xt>

op0 | op1 | CRn | CRm | op2
--- | --- | --- | --- | ---
0b11 | 0b000 | 0b1001 | 0b1001 | 0b110

if PSTATE.EL == EL0 then UNDEFINED; elsif PSTATE.EL == EL1 then if HaveEL(EL3) && EL3SDDUndefPriority() && (MDCR_EL3.NSPB[0] == '0' || MDCR_EL3.NSPB[1] != SCR_EL3.NS || (IsFeatureImplemented(FEAT_RME) && MDCR_EL3.NSPBE != SCR_EL3.NSE)) then UNDEFINED; elsif EL2Enabled() && IsFeatureImplemented(FEAT_FGT) && (!HaveEL(EL3) || SCR_EL3.FGTEn == '1') && HDFGWTR_EL2.PMSLATFR_EL1 == '1' then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && MDCR_EL2.TPMS == '1' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && (MDCR_EL3.NSPB[0] == '0' || MDCR_EL3.NSPB[1] != SCR_EL3.NS || (IsFeatureImplemented(FEAT_RME) && MDCR_EL3.NSPBE != SCR_EL3.NSE)) then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif EffectiveHCR_EL2_NVx() IN {'1x1'} then NVMem[0x848] = X[t, 64]; else PMSLATFR_EL1 = X[t, 64]; elsif PSTATE.EL == EL2 then if HaveEL(EL3) && EL3SDDUndefPriority() && (MDCR_EL3.NSPB[0] == '0' || MDCR_EL3.NSPB[1] != SCR_EL3.NS || (IsFeatureImplemented(FEAT_RME) && MDCR_EL3.NSPBE != SCR_EL3.NSE)) then UNDEFINED; elsif HaveEL(EL3) && (MDCR_EL3.NSPB[0] == '0' || MDCR_EL3.NSPB[1] != SCR_EL3.NS || (IsFeatureImplemented(FEAT_RME) && MDCR_EL3.NSPBE != SCR_EL3.NSE)) then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); else PMSLATFR_EL1 = X[t, 64]; elsif PSTATE.EL == EL3 then PMSLATFR_EL1 = X[t, 64];

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.