Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## BFMLSLT (vectors)

BFloat16 floating-point multiply-subtract long from single-precision (top)

This BFloat16 floating-point multiply-subtract long instruction widens the odd-numbered BFloat16 elements in the first source vector and the corresponding elements in the second source vector to single-precision format and then destructively multiplies and subtracts these values without intermediate rounding from the single-precision elements of the destination vector that overlap with the corresponding BFloat16 elements in the source vectors. This instruction is unpredicated.

### SVE2
(FEAT_SVE2p1)

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | 1 | 1 | 0 | 0 | 1 | 0 | 0 | 1 | 1 | 1 | Zm | 1 | 0 | 1 | 0 | 0 | 1 | Zn | Zda
| o2 |  |  |  | op |  | T |  |

####

BFMLSLT <Zda>.S, <Zn>.H, <Zm>.H

if !IsFeatureImplemented(FEAT_SME2) && !IsFeatureImplemented(FEAT_SVE2p1) then UNDEFINED; constant integer n = UInt(Zn); constant integer m = UInt(Zm); constant integer da = UInt(Zda); constant boolean op1_neg = TRUE;

### Assembler Symbols

<Zda> | Is the name of the third source and destination scalable vector register, encoded in the "Zda" field.

<Zn> | Is the name of the first source scalable vector register, encoded in the "Zn" field.

<Zm> | Is the name of the second source scalable vector register, encoded in the "Zm" field.

### Operation

CheckSVEEnabled(); constant integer VL = CurrentVL; constant integer PL = VL DIV 8; constant integer elements = VL DIV 32; constant bits(VL) op1 = Z[n, VL]; constant bits(VL) op2 = Z[m, VL]; constant bits(VL) op3 = Z[da, VL]; bits(VL) result; for e = 0 to elements-1 constant bits(16) elem1 = (if op1_neg then BFNeg(Elem[op1, 2*e + 1, 16]) else Elem[op1, 2*e + 1, 16]); constant bits(16) elem2 = Elem[op2, 2*e + 1, 16]; constant bits(32) elem3 = Elem[op3, e, 32]; Elem[result, e, 32] = BFMulAddH(elem3, elem1, elem2, FPCR); Z[da, VL] = result;

### Operational information

This instruction might be immediately preceded in program order by a MOVPRFX instruction. The MOVPRFX must conform to all of the following requirements, otherwise the behavior of the MOVPRFX and this instruction is constrained unpredictable:

- The MOVPRFX must be unpredicated.
- The MOVPRFX must specify the same destination register as this instruction.
- The destination register must not refer to architectural register state referenced by any other source operand register of this instruction.

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: aarchmrs v2024-03_relA, pseudocode v2024-03_rel, sve v2024-03_rel ; Build timestamp: 2024-03-26T09:45

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.