AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# PMOVSR, Performance Monitors Overflow Flag Status Register

The PMOVSR characteristics are:

## Purpose

Allows software to clear the unsigned overflow flags for the following counters to 0:

- The cycle counter PMCCNTR.
- The event counters PMEVCNTR<n>.

Reading from this register shows the current unsigned overflow flag values.

## Configuration

AArch32 System register PMOVSR bits [31:0] are architecturally mapped to AArch64 System register PMOVSCLR_EL0[31:0].

AArch32 System register PMOVSR bits [31:0] are architecturally mapped to External register PMU.PMOVSCLR_EL0[31:0].

AArch32 System register PMOVSR bits [31:0] are architecturally mapped to External register PMU.PMOVS[31:0].

This register is present only when AArch32 is supported and FEAT_PMUv3 is implemented. Otherwise, direct accesses to PMOVSR are UNDEFINED.

## Attributes

PMOVSR is a 32-bit register.

## Field descriptions

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
C | P30 | P29 | P28 | P27 | P26 | P25 | P24 | P23 | P22 | P21 | P20 | P19 | P18 | P17 | P16 | P15 | P14 | P13 | P12 | P11 | P10 | P9 | P8 | P7 | P6 | P5 | P4 | P3 | P2 | P1 | P0

#### C, bit [31]

Unsigned overflow flag for PMCCNTR clear. On writes, allows software to clear the unsigned overflow flag for PMCCNTR to 0. On reads, returns the unsigned overflow flag for PMCCNTR overflow status.

C | Meaning
--- | ---
0b0 | PMCCNTR has not overflowed.
0b1 | PMCCNTR has overflowed.

PMCR.LC controls whether an overflow is detected from unsigned overflow of PMCCNTR[31:0] or unsigned overflow of PMCCNTR[63:0].

Accessing this field has the following behavior:

- Permitted reads and writes of this field are RAZ/WI if all of the following are true:
  - FEAT_PMUv3p9 is implemented.
  - Accessed at EL0.
  - EL1 is using AArch64.
  - PMUSERENR_EL0.UEN == 1.
  - PMUACR_EL1.C == 0.
- Permitted writes of this field are ignored if all of the following are true:
  - FEAT_PMUv3p9 is implemented.
  - Accessed at EL0.
  - EL1 is using AArch64.
  - PMUSERENR_EL0.{UEN,CR} == {1,1}.
- Otherwise access to this field is W1C.

The reset behavior of this field is:

- On a Warm reset, this field resets to an architecturally UNKNOWN value.

#### P<m>, bit [m], for m = 30 to 0

Unsigned overflow flag for PMEVCNTR<m> clear. On writes, allows software to clear the unsigned overflow flag for PMEVCNTR<m> to 0. On reads, returns the unsigned overflow flag for PMEVCNTR<m> overflow status.

P<m> | Meaning
--- | ---
0b0 | PMEVCNTR<m> has not overflowed.
0b1 | PMEVCNTR<m> has overflowed.

If FEAT_PMUv3p5 is implemented, MDCR_EL2.HLP, HDCR.HLP, and PMCR.LP control whether an overflow is detected from unsigned overflow of PMEVCNTR<m>[31:0] or unsigned overflow of PMEVCNTR<m>[63:0].

Accessing this field has the following behavior:

- Permitted reads and writes of this field are RAZ/WI if any of the following are true:
  - All of the following are true:
    - FEAT_PMUv3p9 is implemented.
    - Accessed at EL0.
    - EL1 is using AArch64.
    - PMUSERENR_EL0.UEN == 1.
    - PMUACR_EL1.P<m> == 0.
  - All of the following are true:
    - EL2 is implemented and enabled in the current Security state.
    - m >= UInt(MDCR_EL2.HPMN).
    - EL2 using AArch64.
    - Accessed at EL0 or EL1.
  - All of the following are true:
    - EL2 is implemented and enabled in the current Security state.
    - m >= UInt(HDCR.HPMN).
    - EL2 using AArch32.
    - Accessed at EL0 or EL1.
  - m >= UInt(PMCR.N).
- Permitted writes of this field are ignored if all of the following are true:
  - FEAT_PMUv3p9 is implemented.
  - Accessed at EL0.
  - EL1 is using AArch64.
  - PMUSERENR_EL0.{UEN,ER} == {1,1}.
- Otherwise access to this field is W1C.

The reset behavior of this field is:

- On a Warm reset, this field resets to an architecturally UNKNOWN value.

## Accessing PMOVSR

Accesses to this register use the following encodings in the System register encoding space:

#### MRC{<c>}{<q>} <coproc>, {#}<opc1>, <Rt>, <CRn>, <CRm>{, {#}<opc2>}

coproc | opc1 | CRn | CRm | opc2
--- | --- | --- | --- | ---
0b1111 | 0b000 | 0b1001 | 0b1100 | 0b011

if PSTATE.EL == EL0 then if HaveEL(EL3) && EL3SDDUndefPriority() && !ELUsingAArch32(EL3) && MDCR_EL3.TPM == '1' then UNDEFINED; elsif !ELUsingAArch32(EL1) && (PMUSERENR_EL0.EN == '0' && (!IsFeatureImplemented(FEAT_PMUv3p9) || PMUSERENR_EL0.UEN == '0')) then if EL2Enabled() && !ELUsingAArch32(EL2) && HCR_EL2.TGE == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); else AArch64.AArch32SystemAccessTrap(EL1, 0x03); elsif ELUsingAArch32(EL1) && PMUSERENR.EN == '0' then if EL2Enabled() && !ELUsingAArch32(EL2) && HCR_EL2.TGE == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HCR.TGE == '1' then AArch32.TakeHypTrapException(0x00); else UNDEFINED; elsif EL2Enabled() && !ELUsingAArch32(EL2) && !ELIsInHost(EL0) && HSTR_EL2.T9 == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HSTR.T9 == '1' then AArch32.TakeHypTrapException(0x03); elsif EL2Enabled() && !ELUsingAArch32(EL1) && !ELIsInHost(EL0) && IsFeatureImplemented(FEAT_FGT) && (!HaveEL(EL3) || SCR_EL3.FGTEn == '1') && HDFGRTR_EL2.PMOVS == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && !ELUsingAArch32(EL2) && MDCR_EL2.TPM == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HDCR.TPM == '1' then AArch32.TakeHypTrapException(0x03); elsif HaveEL(EL3) && !ELUsingAArch32(EL3) && MDCR_EL3.TPM == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.AArch32SystemAccessTrap(EL3, 0x03); else R[t] = PMOVSR; elsif PSTATE.EL == EL1 then if HaveEL(EL3) && EL3SDDUndefPriority() && !ELUsingAArch32(EL3) && MDCR_EL3.TPM == '1' then UNDEFINED; elsif EL2Enabled() && !ELUsingAArch32(EL2) && HSTR_EL2.T9 == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HSTR.T9 == '1' then AArch32.TakeHypTrapException(0x03); elsif EL2Enabled() && !ELUsingAArch32(EL2) && MDCR_EL2.TPM == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HDCR.TPM == '1' then AArch32.TakeHypTrapException(0x03); elsif HaveEL(EL3) && !ELUsingAArch32(EL3) && MDCR_EL3.TPM == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.AArch32SystemAccessTrap(EL3, 0x03); else R[t] = PMOVSR; elsif PSTATE.EL == EL2 then if HaveEL(EL3) && EL3SDDUndefPriority() && !ELUsingAArch32(EL3) && MDCR_EL3.TPM == '1' then UNDEFINED; elsif HaveEL(EL3) && !ELUsingAArch32(EL3) && MDCR_EL3.TPM == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.AArch32SystemAccessTrap(EL3, 0x03); else R[t] = PMOVSR; elsif PSTATE.EL == EL3 then R[t] = PMOVSR;

#### MCR{<c>}{<q>} <coproc>, {#}<opc1>, <Rt>, <CRn>, <CRm>{, {#}<opc2>}

coproc | opc1 | CRn | CRm | opc2
--- | --- | --- | --- | ---
0b1111 | 0b000 | 0b1001 | 0b1100 | 0b011

if PSTATE.EL == EL0 then if HaveEL(EL3) && EL3SDDUndefPriority() && !ELUsingAArch32(EL3) && MDCR_EL3.TPM == '1' then UNDEFINED; elsif !ELUsingAArch32(EL1) && (PMUSERENR_EL0.EN == '0' && (!IsFeatureImplemented(FEAT_PMUv3p9) || PMUSERENR_EL0.UEN == '0')) then if EL2Enabled() && !ELUsingAArch32(EL2) && HCR_EL2.TGE == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); else AArch64.AArch32SystemAccessTrap(EL1, 0x03); elsif ELUsingAArch32(EL1) && PMUSERENR.EN == '0' then if EL2Enabled() && !ELUsingAArch32(EL2) && HCR_EL2.TGE == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HCR.TGE == '1' then AArch32.TakeHypTrapException(0x00); else UNDEFINED; elsif EL2Enabled() && !ELUsingAArch32(EL2) && !ELIsInHost(EL0) && HSTR_EL2.T9 == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HSTR.T9 == '1' then AArch32.TakeHypTrapException(0x03); elsif EL2Enabled() && !ELUsingAArch32(EL1) && !ELIsInHost(EL0) && IsFeatureImplemented(FEAT_FGT) && (!HaveEL(EL3) || SCR_EL3.FGTEn == '1') && HDFGWTR_EL2.PMOVS == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && !ELUsingAArch32(EL2) && MDCR_EL2.TPM == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HDCR.TPM == '1' then AArch32.TakeHypTrapException(0x03); elsif HaveEL(EL3) && !ELUsingAArch32(EL3) && MDCR_EL3.TPM == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.AArch32SystemAccessTrap(EL3, 0x03); else PMOVSR = R[t]; elsif PSTATE.EL == EL1 then if HaveEL(EL3) && EL3SDDUndefPriority() && !ELUsingAArch32(EL3) && MDCR_EL3.TPM == '1' then UNDEFINED; elsif EL2Enabled() && !ELUsingAArch32(EL2) && HSTR_EL2.T9 == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HSTR.T9 == '1' then AArch32.TakeHypTrapException(0x03); elsif EL2Enabled() && !ELUsingAArch32(EL2) && MDCR_EL2.TPM == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HDCR.TPM == '1' then AArch32.TakeHypTrapException(0x03); elsif HaveEL(EL3) && !ELUsingAArch32(EL3) && MDCR_EL3.TPM == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.AArch32SystemAccessTrap(EL3, 0x03); else PMOVSR = R[t]; elsif PSTATE.EL == EL2 then if HaveEL(EL3) && EL3SDDUndefPriority() && !ELUsingAArch32(EL3) && MDCR_EL3.TPM == '1' then UNDEFINED; elsif HaveEL(EL3) && !ELUsingAArch32(EL3) && MDCR_EL3.TPM == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.AArch32SystemAccessTrap(EL3, 0x03); else PMOVSR = R[t]; elsif PSTATE.EL == EL3 then PMOVSR = R[t];

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.