Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## UCLAMP

Multi-vector unsigned clamp to minimum/maximum vector

Clamp each unsigned element in the two or four destination vectors to between the unsigned minimum value in the corresponding element of the first source vector and the unsigned maximum value in the corresponding element of the second source vector and destructively place the clamped results in the corresponding elements of the two or four destination vectors.

This instruction is unpredicated.

It has encodings from 2 classes: Two registers and Four registers

### Two registers
(FEAT_SME2)

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
1 | 1 | 0 | 0 | 0 | 0 | 0 | 1 | size | 1 | Zm | 1 | 1 | 0 | 0 | 0 | 1 | Zn | Zd | 1
|  |  |  |  |  |  | U

####

UCLAMP { <Zd1>.<T>-<Zd2>.<T> }, <Zn>.<T>, <Zm>.<T>

if !HaveSME2() then UNDEFINED; constant integer esize = 8 << UInt(size); integer n = UInt(Zn); integer m = UInt(Zm); integer d = UInt(Zd:'0'); constant integer nreg = 2;

### Four registers
(FEAT_SME2)

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
1 | 1 | 0 | 0 | 0 | 0 | 0 | 1 | size | 1 | Zm | 1 | 1 | 0 | 0 | 1 | 1 | Zn | Zd | 0 | 1
|  |  |  |  |  |  |  | U

####

UCLAMP { <Zd1>.<T>-<Zd4>.<T> }, <Zn>.<T>, <Zm>.<T>

if !HaveSME2() then UNDEFINED; constant integer esize = 8 << UInt(size); integer n = UInt(Zn); integer m = UInt(Zm); integer d = UInt(Zd:'00'); constant integer nreg = 4;

### Assembler Symbols

<Zd1> | For the two registers variant: is the name of the first destination scalable vector register of a multi-vector sequence, encoded as "Zd" times 2.
| For the four registers variant: is the name of the first destination scalable vector register of a multi-vector sequence, encoded as "Zd" times 4.

<T> | Is the size specifier, encoded in size:
size | <T>
--- | ---
00 | B
01 | H
10 | S
11 | D

<Zd4> | Is the name of the fourth destination scalable vector register of a multi-vector sequence, encoded as "Zd" times 4 plus 3.

<Zd2> | Is the name of the second destination scalable vector register of a multi-vector sequence, encoded as "Zd" times 2 plus 1.

<Zn> | Is the name of the first source scalable vector register, encoded in the "Zn" field.

<Zm> | Is the name of the second source scalable vector register, encoded in the "Zm" field.

### Operation

CheckStreamingSVEEnabled(); constant integer VL = CurrentVL; constant integer elements = VL DIV esize; array [0..3] of bits(VL) results; for r = 0 to nreg-1 bits(VL) operand1 = Z[n, VL]; bits(VL) operand2 = Z[m, VL]; bits(VL) operand3 = Z[d+r, VL]; for e = 0 to elements-1 integer element1 = UInt(Elem[operand1, e, esize]); integer element2 = UInt(Elem[operand2, e, esize]); integer element3 = UInt(Elem[operand3, e, esize]); integer res = Min(Max(element1, element3), element2); Elem[results[r], e, esize] = res<esize-1:0>; for r = 0 to nreg-1 Z[d+r, VL] = results[r];

### Operational information

If PSTATE.DIT is 1:

- The execution time of this instruction is independent of:
  - The values of the data supplied in any of its registers.
  - The values of the NZCV flags.
- The response of this instruction to asynchronous exceptions does not vary based on:
  - The values of the data supplied in any of its registers.
  - The values of the NZCV flags.

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: isa v33.64, AdvSIMD v29.12, pseudocode v2023-06_rel, sve v2023-06_rel ; Build timestamp: 2023-07-04T19:42

Copyright © 2010-2023 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.