Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## UQADD

Unsigned saturating Add. This instruction adds the values of corresponding elements of the two source SIMD&FP registers, places the results into a vector, and writes the vector to the destination SIMD&FP register.

If overflow occurs with any of the results, those results are saturated. If saturation occurs, the cumulative saturation bit FPSR.QC is set.

Depending on the settings in the CPACR_EL1, CPTR_EL2, and CPTR_EL3 registers, and the current Security state and Exception level, an attempt to execute the instruction might be trapped.

It has encodings from 2 classes: Scalar and Vector

### Scalar

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | 1 | 1 | 1 | 1 | 1 | 1 | 0 | size | 1 | Rm | 0 | 0 | 0 | 0 | 1 | 1 | Rn | Rd
| U |  |  |  |  | opcode |  |  |

####

UQADD <V><d>, <V><n>, <V><m>

integer d = UInt(Rd); integer n = UInt(Rn); integer m = UInt(Rm); constant integer esize = 8 << UInt(size); constant integer datasize = esize; integer elements = 1; boolean unsigned = (U == '1');

### Vector

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | Q | 1 | 0 | 1 | 1 | 1 | 0 | size | 1 | Rm | 0 | 0 | 0 | 0 | 1 | 1 | Rn | Rd
|  | U |  |  |  |  | opcode |  |  |

####

UQADD <Vd>.<T>, <Vn>.<T>, <Vm>.<T>

integer d = UInt(Rd); integer n = UInt(Rn); integer m = UInt(Rm); if size:Q == '110' then UNDEFINED; constant integer esize = 8 << UInt(size); constant integer datasize = 64 << UInt(Q); integer elements = datasize DIV esize; boolean unsigned = (U == '1');

### Assembler Symbols

<V> | Is a width specifier, encoded in size:
size | <V>
--- | ---
00 | B
01 | H
10 | S
11 | D

<d> | Is the number of the SIMD&FP destination register, in the "Rd" field.

<n> | Is the number of the first SIMD&FP source register, encoded in the "Rn" field.

<m> | Is the number of the second SIMD&FP source register, encoded in the "Rm" field.

<Vd> | Is the name of the SIMD&FP destination register, encoded in the "Rd" field.

<T> | Is an arrangement specifier, encoded in size:Q:
size | Q | <T>
--- | --- | ---
00 | 0 | 8B
00 | 1 | 16B
01 | 0 | 4H
01 | 1 | 8H
10 | 0 | 2S
10 | 1 | 4S
11 | 0 | RESERVED
11 | 1 | 2D

<Vn> | Is the name of the first SIMD&FP source register, encoded in the "Rn" field.

<Vm> | Is the name of the second SIMD&FP source register, encoded in the "Rm" field.

### Operation

CheckFPAdvSIMDEnabled64(); bits(datasize) operand1 = V[n, datasize]; bits(datasize) operand2 = V[m, datasize]; bits(datasize) result; integer element1; integer element2; integer sum; boolean sat; for e = 0 to elements-1 element1 = Int(Elem[operand1, e, esize], unsigned); element2 = Int(Elem[operand2, e, esize], unsigned); sum = element1 + element2; (Elem[result, e, esize], sat) = SatQ(sum, esize, unsigned); if sat then FPSR.QC = '1'; V[d, datasize] = result;

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: aarchmrs v2024-03_relA, pseudocode v2024-03_rel, sve v2024-03_rel ; Build timestamp: 2024-03-26T09:45

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.