AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# HAIFSR, Hyp Auxiliary Instruction Fault Status Register

The HAIFSR characteristics are:

## Purpose

Provides additional IMPLEMENTATION DEFINED syndrome information for Prefetch Abort exceptions taken to Hyp mode.

## Configuration

AArch32 System register HAIFSR bits [31:0] are architecturally mapped to AArch64 System register AFSR1_EL2[31:0].

This register is present only when EL2 is capable of using AArch32. Otherwise, direct accesses to HAIFSR are UNDEFINED.

This is an optional register. An implementation that does not require this register can implement it as RES0.

If EL2 is not implemented, this register is RES0 from EL3.

## Attributes

HAIFSR is a 32-bit register.

## Field descriptions

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
IMPLEMENTATION DEFINED

#### IMPLEMENTATION DEFINED, bits [31:0]

IMPLEMENTATION DEFINED.

The reset behavior of this field is:

- On a Warm reset, this field resets to an architecturally UNKNOWN value.

## Accessing HAIFSR

Accesses to this register use the following encodings in the System register encoding space:

#### MRC{<c>}{<q>} <coproc>, {#}<opc1>, <Rt>, <CRn>, <CRm>{, {#}<opc2>}

coproc | opc1 | CRn | CRm | opc2
--- | --- | --- | --- | ---
0b1111 | 0b100 | 0b0101 | 0b0001 | 0b001

if PSTATE.EL == EL0 then UNDEFINED; elsif PSTATE.EL == EL1 then if EL2Enabled() && !ELUsingAArch32(EL2) && HSTR_EL2.T5 == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HSTR.T5 == '1' then AArch32.TakeHypTrapException(0x03); else UNDEFINED; elsif PSTATE.EL == EL2 then R[t] = HAIFSR; elsif PSTATE.EL == EL3 then if SCR.NS == '0' then UNDEFINED; else R[t] = HAIFSR;

#### MCR{<c>}{<q>} <coproc>, {#}<opc1>, <Rt>, <CRn>, <CRm>{, {#}<opc2>}

coproc | opc1 | CRn | CRm | opc2
--- | --- | --- | --- | ---
0b1111 | 0b100 | 0b0101 | 0b0001 | 0b001

if PSTATE.EL == EL0 then UNDEFINED; elsif PSTATE.EL == EL1 then if EL2Enabled() && !ELUsingAArch32(EL2) && HSTR_EL2.T5 == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HSTR.T5 == '1' then AArch32.TakeHypTrapException(0x03); else UNDEFINED; elsif PSTATE.EL == EL2 then HAIFSR = R[t]; elsif PSTATE.EL == EL3 then if SCR.NS == '0' then UNDEFINED; else HAIFSR = R[t];

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.