AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# SPMOVSCLR_EL0, System Performance Monitors Overflow Flag Status Clear Register

The SPMOVSCLR_EL0 characteristics are:

## Purpose

Clears the state of overflow bits for event counters in System PMU <s>.

## Configuration

This register is present only when FEAT_SPMU is implemented. Otherwise, direct accesses to SPMOVSCLR_EL0 are UNDEFINED.

## Attributes

SPMOVSCLR_EL0 is a 64-bit register.

## Field descriptions

63 | 62 | 61 | 60 | 59 | 58 | 57 | 56 | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48 | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40 | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
P63 | P62 | P61 | P60 | P59 | P58 | P57 | P56 | P55 | P54 | P53 | P52 | P51 | P50 | P49 | P48 | P47 | P46 | P45 | P44 | P43 | P42 | P41 | P40 | P39 | P38 | P37 | P36 | P35 | P34 | P33 | P32
P31 | P30 | P29 | P28 | P27 | P26 | P25 | P24 | P23 | P22 | P21 | P20 | P19 | P18 | P17 | P16 | P15 | P14 | P13 | P12 | P11 | P10 | P9 | P8 | P7 | P6 | P5 | P4 | P3 | P2 | P1 | P0

#### P<m>, bit [m], for m = 63 to 0

Event counter <m> unsigned overflow bit clear.

P<m> | Meaning
--- | ---
0b0 | Event counter <m> in System PMU <s> has not overflowed.
0b1 | Event counter <m> in System PMU <s> has overflowed.

The reset behavior of this field is:

- On a System PMU reset, this field resets to an architecturally UNKNOWN value.

Accessing this field has the following behavior:

- Access is RAZ/WI if event counter <m> is not implemented by System PMU <s> or event counter <m> does not implement an overflow flag.
- Otherwise, access to this field is W1C.

## Accessing SPMOVSCLR_EL0

To access SPMOVSCLR_EL0 for System PMU <s>, set SPMSELR_EL0.SYSPMUSEL to s.

SPMOVSCLR_EL0 reads-as-zero and ignores writes if System PMU <s> is not implemented.

Accesses to this register use the following encodings in the System register encoding space:

#### MRS <Xt>, SPMOVSCLR_EL0

op0 | op1 | CRn | CRm | op2
--- | --- | --- | --- | ---
0b10 | 0b011 | 0b1001 | 0b1100 | 0b011

if PSTATE.EL == EL0 then if HaveEL(EL3) && EL3SDDUndefPriority() && MDCR_EL3.EnPM2 == '0' then UNDEFINED; elsif HaveEL(EL3) && EL3SDDUndefPriority() && SPMACCESSR_EL3<(UInt(SPMSELR_EL0.SYSPMUSEL) * 2) + 1:UInt(SPMSELR_EL0.SYSPMUSEL) * 2> == '00' then UNDEFINED; elsif MDSCR_EL1.EnSPM == '0' then if EL2Enabled() && HCR_EL2.TGE == '1' then AArch64.SystemAccessTrap(EL2, 0x18); else AArch64.SystemAccessTrap(EL1, 0x18); elsif !ELIsInHost(EL0) && SPMACCESSR_EL1<(UInt(SPMSELR_EL0.SYSPMUSEL) * 2) + 1:UInt(SPMSELR_EL0.SYSPMUSEL) * 2> == '00' then if EL2Enabled() && HCR_EL2.TGE == '1' then AArch64.SystemAccessTrap(EL2, 0x18); else AArch64.SystemAccessTrap(EL1, 0x18); elsif EL2Enabled() && !ELIsInHost(EL0) && IsFeatureImplemented(FEAT_FGT2) && HaveEL(EL3) && SCR_EL3.FGTEn2 == '0' then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && !ELIsInHost(EL0) && IsFeatureImplemented(FEAT_FGT2) && HDFGRTR2_EL2.nSPMOVS == '0' then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && MDCR_EL2.EnSPM == '0' then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && SPMACCESSR_EL2<(UInt(SPMSELR_EL0.SYSPMUSEL) * 2) + 1:UInt(SPMSELR_EL0.SYSPMUSEL) * 2> == '00' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && MDCR_EL3.EnPM2 == '0' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif HaveEL(EL3) && SPMACCESSR_EL3<(UInt(SPMSELR_EL0.SYSPMUSEL) * 2) + 1:UInt(SPMSELR_EL0.SYSPMUSEL) * 2> == '00' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); else X[t, 64] = SPMOVSCLR_EL0[UInt(SPMSELR_EL0.SYSPMUSEL)]; elsif PSTATE.EL == EL1 then if HaveEL(EL3) && EL3SDDUndefPriority() && MDCR_EL3.EnPM2 == '0' then UNDEFINED; elsif HaveEL(EL3) && EL3SDDUndefPriority() && SPMACCESSR_EL3<(UInt(SPMSELR_EL0.SYSPMUSEL) * 2) + 1:UInt(SPMSELR_EL0.SYSPMUSEL) * 2> == '00' then UNDEFINED; elsif EL2Enabled() && IsFeatureImplemented(FEAT_FGT2) && ((HaveEL(EL3) && SCR_EL3.FGTEn2 == '0') || HDFGRTR2_EL2.nSPMOVS == '0') then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && MDCR_EL2.EnSPM == '0' then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && SPMACCESSR_EL2<(UInt(SPMSELR_EL0.SYSPMUSEL) * 2) + 1:UInt(SPMSELR_EL0.SYSPMUSEL) * 2> == '00' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && MDCR_EL3.EnPM2 == '0' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif HaveEL(EL3) && SPMACCESSR_EL3<(UInt(SPMSELR_EL0.SYSPMUSEL) * 2) + 1:UInt(SPMSELR_EL0.SYSPMUSEL) * 2> == '00' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); else X[t, 64] = SPMOVSCLR_EL0[UInt(SPMSELR_EL0.SYSPMUSEL)]; elsif PSTATE.EL == EL2 then if HaveEL(EL3) && EL3SDDUndefPriority() && MDCR_EL3.EnPM2 == '0' then UNDEFINED; elsif HaveEL(EL3) && EL3SDDUndefPriority() && SPMACCESSR_EL3<(UInt(SPMSELR_EL0.SYSPMUSEL) * 2) + 1:UInt(SPMSELR_EL0.SYSPMUSEL) * 2> == '00' then UNDEFINED; elsif HaveEL(EL3) && MDCR_EL3.EnPM2 == '0' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif HaveEL(EL3) && SPMACCESSR_EL3<(UInt(SPMSELR_EL0.SYSPMUSEL) * 2) + 1:UInt(SPMSELR_EL0.SYSPMUSEL) * 2> == '00' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); else X[t, 64] = SPMOVSCLR_EL0[UInt(SPMSELR_EL0.SYSPMUSEL)]; elsif PSTATE.EL == EL3 then X[t, 64] = SPMOVSCLR_EL0[UInt(SPMSELR_EL0.SYSPMUSEL)];

#### MSR SPMOVSCLR_EL0, <Xt>

op0 | op1 | CRn | CRm | op2
--- | --- | --- | --- | ---
0b10 | 0b011 | 0b1001 | 0b1100 | 0b011

if PSTATE.EL == EL0 then if HaveEL(EL3) && EL3SDDUndefPriority() && MDCR_EL3.EnPM2 == '0' then UNDEFINED; elsif HaveEL(EL3) && EL3SDDUndefPriority() && SPMACCESSR_EL3<(UInt(SPMSELR_EL0.SYSPMUSEL) * 2) + 1:UInt(SPMSELR_EL0.SYSPMUSEL) * 2> != '11' then UNDEFINED; elsif MDSCR_EL1.EnSPM == '0' then if EL2Enabled() && HCR_EL2.TGE == '1' then AArch64.SystemAccessTrap(EL2, 0x18); else AArch64.SystemAccessTrap(EL1, 0x18); elsif !ELIsInHost(EL0) && SPMACCESSR_EL1<(UInt(SPMSELR_EL0.SYSPMUSEL) * 2) + 1:UInt(SPMSELR_EL0.SYSPMUSEL) * 2> != '11' then if EL2Enabled() && HCR_EL2.TGE == '1' then AArch64.SystemAccessTrap(EL2, 0x18); else AArch64.SystemAccessTrap(EL1, 0x18); elsif EL2Enabled() && !ELIsInHost(EL0) && IsFeatureImplemented(FEAT_FGT2) && HaveEL(EL3) && SCR_EL3.FGTEn2 == '0' then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && !ELIsInHost(EL0) && IsFeatureImplemented(FEAT_FGT2) && HDFGWTR2_EL2.nSPMOVS == '0' then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && MDCR_EL2.EnSPM == '0' then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && SPMACCESSR_EL2<(UInt(SPMSELR_EL0.SYSPMUSEL) * 2) + 1:UInt(SPMSELR_EL0.SYSPMUSEL) * 2> != '11' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && MDCR_EL3.EnPM2 == '0' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif HaveEL(EL3) && SPMACCESSR_EL3<(UInt(SPMSELR_EL0.SYSPMUSEL) * 2) + 1:UInt(SPMSELR_EL0.SYSPMUSEL) * 2> != '11' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); else SPMOVSCLR_EL0[UInt(SPMSELR_EL0.SYSPMUSEL)] = X[t, 64]; elsif PSTATE.EL == EL1 then if HaveEL(EL3) && EL3SDDUndefPriority() && MDCR_EL3.EnPM2 == '0' then UNDEFINED; elsif HaveEL(EL3) && EL3SDDUndefPriority() && SPMACCESSR_EL3<(UInt(SPMSELR_EL0.SYSPMUSEL) * 2) + 1:UInt(SPMSELR_EL0.SYSPMUSEL) * 2> != '11' then UNDEFINED; elsif EL2Enabled() && IsFeatureImplemented(FEAT_FGT2) && ((HaveEL(EL3) && SCR_EL3.FGTEn2 == '0') || HDFGWTR2_EL2.nSPMOVS == '0') then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && MDCR_EL2.EnSPM == '0' then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && SPMACCESSR_EL2<(UInt(SPMSELR_EL0.SYSPMUSEL) * 2) + 1:UInt(SPMSELR_EL0.SYSPMUSEL) * 2> != '11' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && MDCR_EL3.EnPM2 == '0' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif HaveEL(EL3) && SPMACCESSR_EL3<(UInt(SPMSELR_EL0.SYSPMUSEL) * 2) + 1:UInt(SPMSELR_EL0.SYSPMUSEL) * 2> != '11' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); else SPMOVSCLR_EL0[UInt(SPMSELR_EL0.SYSPMUSEL)] = X[t, 64]; elsif PSTATE.EL == EL2 then if HaveEL(EL3) && EL3SDDUndefPriority() && MDCR_EL3.EnPM2 == '0' then UNDEFINED; elsif HaveEL(EL3) && EL3SDDUndefPriority() && SPMACCESSR_EL3<(UInt(SPMSELR_EL0.SYSPMUSEL) * 2) + 1:UInt(SPMSELR_EL0.SYSPMUSEL) * 2> != '11' then UNDEFINED; elsif HaveEL(EL3) && MDCR_EL3.EnPM2 == '0' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif HaveEL(EL3) && SPMACCESSR_EL3<(UInt(SPMSELR_EL0.SYSPMUSEL) * 2) + 1:UInt(SPMSELR_EL0.SYSPMUSEL) * 2> != '11' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); else SPMOVSCLR_EL0[UInt(SPMSELR_EL0.SYSPMUSEL)] = X[t, 64]; elsif PSTATE.EL == EL3 then SPMOVSCLR_EL0[UInt(SPMSELR_EL0.SYSPMUSEL)] = X[t, 64];

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.