Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## ASR (immediate)

Arithmetic Shift Right (immediate) shifts a register value right by an immediate number of bits, shifting in copies of the sign bit in the upper bits and zeros in the lower bits, and writes the result to the destination register.

This is an alias of SBFM. This means:

- The encodings in this description are named to match the encodings of SBFM.
- The description of SBFM gives the operational pseudocode, any constrained unpredictable behavior, and any operational information for this instruction.

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
sf | 0 | 0 | 1 | 0 | 0 | 1 | 1 | 0 | N | immr | x | 1 | 1 | 1 | 1 | 1 | Rn | Rd
| opc |  |  |  | imms |  |

#### 32-bit (sf == 0 && N == 0 && imms == 011111)

ASR <Wd>, <Wn>, #<shift>

is equivalent to

SBFM <Wd>, <Wn>, #<shift>, #31

and is always the preferred disassembly.

#### 64-bit (sf == 1 && N == 1 && imms == 111111)

ASR <Xd>, <Xn>, #<shift>

is equivalent to

SBFM <Xd>, <Xn>, #<shift>, #63

and is always the preferred disassembly.

### Assembler Symbols

<Wd> | Is the 32-bit name of the general-purpose destination register, encoded in the "Rd" field.

<Wn> | Is the 32-bit name of the general-purpose source register, encoded in the "Rn" field.

<Xd> | Is the 64-bit name of the general-purpose destination register, encoded in the "Rd" field.

<Xn> | Is the 64-bit name of the general-purpose source register, encoded in the "Rn" field.

<shift> | For the 32-bit variant: is the shift amount, in the range 0 to 31, encoded in the "immr" field.
| For the 64-bit variant: is the shift amount, in the range 0 to 63, encoded in the "immr" field.

### Operation

The description of SBFM gives the operational pseudocode for this instruction.

### Operational information

If PSTATE.DIT is 1:

- The execution time of this instruction is independent of:
  - The values of the data supplied in any of its registers.
  - The values of the NZCV flags.
- The response of this instruction to asynchronous exceptions does not vary based on:
  - The values of the data supplied in any of its registers.
  - The values of the NZCV flags.

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: isa v33.74, AdvSIMD v29.23, pseudocode v2023-09_rel, sve v2023-09_rc3 ; Build timestamp: 2023-09-27T17:06

Copyright © 2010-2023 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.