AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# DBGAUTHSTATUS_EL1, Debug Authentication Status Register

The DBGAUTHSTATUS_EL1 characteristics are:

## Purpose

Provides information about the state of the IMPLEMENTATION DEFINED authentication interface for debug.

## Configuration

External register DBGAUTHSTATUS_EL1 bits [31:0] are architecturally mapped to AArch64 System register DBGAUTHSTATUS_EL1[31:0].

External register DBGAUTHSTATUS_EL1 bits [31:0] are architecturally mapped to AArch32 System register DBGAUTHSTATUS[31:0].

When FEAT_DoPD is implemented, DBGAUTHSTATUS_EL1 is in the Core power domain. Otherwise, DBGAUTHSTATUS_EL1 is in the Debug power domain.

## Attributes

DBGAUTHSTATUS_EL1 is a 32-bit register.

## Field descriptions

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
RES0 | RTNID | RTID | RES0 | RLNID | RLID | RES0 | SNID | SID | NSNID | NSID

#### Bits [31:28]

Reserved, RES0.

#### RTNID, bits [27:26]

Root non-invasive debug.

This field has the same value as DBGAUTHSTATUS_EL1.RTID.

This field has an IMPLEMENTATION DEFINED value.

Access to this field is RO.

#### RTID, bits [25:24]

Root invasive debug.

RTID | Meaning
--- | ---
0b00 | Not implemented.
0b10 | Implemented and disabled. ExternalRootInvasiveDebugEnabled() == FALSE.
0b11 | Implemented and enabled. ExternalRootInvasiveDebugEnabled() == TRUE.

All other values are reserved.

If FEAT_RME is not implemented, the only permitted value is 0b00.

#### Bits [23:16]

Reserved, RES0.

#### RLNID, bits [15:14]

Realm non-invasive debug.

This field has the same value as DBGAUTHSTATUS_EL1.RLID.

This field has an IMPLEMENTATION DEFINED value.

Access to this field is RO.

#### RLID, bits [13:12]

Realm invasive debug.

RLID | Meaning
--- | ---
0b00 | Not implemented.
0b10 | Implemented and disabled. ExternalRealmInvasiveDebugEnabled() == FALSE.
0b11 | Implemented and enabled. ExternalRealmInvasiveDebugEnabled() == TRUE.

All other values are reserved.

If FEAT_RME is not implemented, the only permitted value is 0b00.

#### Bits [11:8]

Reserved, RES0.

#### SNID, bits [7:6]
When FEAT_Debugv8p4 is implemented:

Secure non-invasive debug.

This field has the same value as DBGAUTHSTATUS_EL1.SID.

This field has an IMPLEMENTATION DEFINED value.

Access to this field is RO.

####
Otherwise:

Secure non-invasive debug.

The value of this field is an IMPLEMENTATION DEFINED choice of:

SNID | Meaning
--- | ---
0b00 | Secure state is not implemented.
0b10 | Implemented and disabled. ExternalSecureNoninvasiveDebugEnabled() == FALSE.
0b11 | Implemented and enabled. ExternalSecureNoninvasiveDebugEnabled() == TRUE.

All other values are reserved.

Access to this field is RO.

#### SID, bits [5:4]

Secure invasive debug.

The value of this field is an IMPLEMENTATION DEFINED choice of:

SID | Meaning
--- | ---
0b00 | Secure state is not implemented.
0b10 | Implemented and disabled. ExternalSecureInvasiveDebugEnabled() == FALSE.
0b11 | Implemented and enabled. ExternalSecureInvasiveDebugEnabled() == TRUE.

All other values are reserved.

Access to this field is RO.

#### NSNID, bits [3:2]
When FEAT_Debugv8p4 is implemented:

Non-secure non-invasive debug.

The value of this field is an IMPLEMENTATION DEFINED choice of:

NSNID | Meaning
--- | ---
0b00 | Non-secure state is not implemented.
0b11 | Implemented and enabled. ExternalNoninvasiveDebugEnabled() == TRUE.

If the Effective value of SCR_EL3.NS is 1, or if EL3 is implemented and EL2 is not implemented, this field reads as 0b11.

All other values are reserved.

Access to this field is RO.

####
Otherwise:

Non-secure non-invasive debug.

The value of this field is an IMPLEMENTATION DEFINED choice of:

NSNID | Meaning
--- | ---
0b00 | Non-secure state is not implemented.
0b10 | Implemented and disabled. ExternalNoninvasiveDebugEnabled() == FALSE.
0b11 | Implemented and enabled. ExternalNoninvasiveDebugEnabled() == TRUE.

All other values are reserved.

Access to this field is RO.

#### NSID, bits [1:0]

Non-secure invasive debug.

The value of this field is an IMPLEMENTATION DEFINED choice of:

NSID | Meaning
--- | ---
0b00 | Non-secure state is not implemented.
0b10 | Implemented and disabled. ExternalInvasiveDebugEnabled() == FALSE.
0b11 | Implemented and enabled. ExternalInvasiveDebugEnabled() == TRUE.

All other values are reserved.

Access to this field is RO.

## Accessing DBGAUTHSTATUS_EL1

#### DBGAUTHSTATUS_EL1 can be accessed through the external debug interface:

Component | Offset | Instance
--- | --- | ---
Debug | 0xFB8 | DBGAUTHSTATUS_EL1

This interface is accessible as follows:

- When FEAT_DoPD is implemented and !IsCorePowered(), accesses to this register generate an error response.
- Otherwise, accesses to this register are RO.

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.