Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## SMLSL, SMLSL2 (vector)

Signed Multiply-Subtract Long (vector). This instruction multiplies corresponding signed integer values in the lower or upper half of the vectors of the two source SIMD&FP registers, and subtracts the results from the vector elements of the destination SIMD&FP register. The destination vector elements are twice as long as the elements that are multiplied.

The SMLSL instruction extracts each source vector from the lower half of each source register. The SMLSL2 instruction extracts each source vector from the upper half of each source register.

Depending on the settings in the CPACR_EL1, CPTR_EL2, and CPTR_EL3 registers, and the current Security state and Exception level, an attempt to execute the instruction might be trapped.

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | Q | 0 | 0 | 1 | 1 | 1 | 0 | size | 1 | Rm | 1 | 0 | 1 | 0 | 0 | 0 | Rn | Rd
|  | U |  |  |  |  |  | o1 |  |  |  |

####

SMLSL{2} <Vd>.<Ta>, <Vn>.<Tb>, <Vm>.<Tb>

integer d = UInt(Rd); integer n = UInt(Rn); integer m = UInt(Rm); if size == '11' then UNDEFINED; constant integer esize = 8 << UInt(size); constant integer datasize = 64; integer part = UInt(Q); integer elements = datasize DIV esize; boolean sub_op = (o1 == '1'); boolean unsigned = (U == '1');

### Assembler Symbols

2 | Is the second and upper half specifier. If present it causes the operation to be performed on the upper 64 bits of the registers holding the narrower elements, and is encoded in Q:
Q | 2
--- | ---
0 | [absent]
1 | [present]

<Vd> | Is the name of the SIMD&FP destination register, encoded in the "Rd" field.

<Ta> | Is an arrangement specifier, encoded in size:
size | <Ta>
--- | ---
00 | 8H
01 | 4S
10 | 2D
11 | RESERVED

<Vn> | Is the name of the first SIMD&FP source register, encoded in the "Rn" field.

<Tb> | Is an arrangement specifier, encoded in size:Q:
size | Q | <Tb>
--- | --- | ---
00 | 0 | 8B
00 | 1 | 16B
01 | 0 | 4H
01 | 1 | 8H
10 | 0 | 2S
10 | 1 | 4S
11 | x | RESERVED

<Vm> | Is the name of the second SIMD&FP source register, encoded in the "Rm" field.

### Operation

CheckFPAdvSIMDEnabled64(); bits(datasize) operand1 = Vpart[n, part, datasize]; bits(datasize) operand2 = Vpart[m, part, datasize]; bits(2*datasize) operand3 = V[d, 2*datasize]; bits(2*datasize) result; integer element1; integer element2; bits(2*esize) product; bits(2*esize) accum; for e = 0 to elements-1 element1 = Int(Elem[operand1, e, esize], unsigned); element2 = Int(Elem[operand2, e, esize], unsigned); product = (element1*element2)<2*esize-1:0>; if sub_op then accum = Elem[operand3, e, 2*esize] - product; else accum = Elem[operand3, e, 2*esize] + product; Elem[result, e, 2*esize] = accum; V[d, 2*datasize] = result;

### Operational information

If PSTATE.DIT is 1:

- The execution time of this instruction is independent of:
  - The values of the data supplied in any of its registers.
  - The values of the NZCV flags.
- The response of this instruction to asynchronous exceptions does not vary based on:
  - The values of the data supplied in any of its registers.
  - The values of the NZCV flags.

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: isa v33.74, AdvSIMD v29.23, pseudocode v2023-09_rel, sve v2023-09_rc3 ; Build timestamp: 2023-09-27T17:06

Copyright © 2010-2023 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.