Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## SQRDMLAH (vectors)

Signed saturating rounding doubling multiply-add high to accumulator (unpredicated)

Multiply then double the corresponding signed elements of the first and second source vectors, and destructively add the rounded high half of each result to the corresponding elements of the addend and destination vector. Each destination element is saturated to the N-bit element's signed integer range -2(N-1) to (2(N-1) )-1. This instruction is unpredicated.

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | 1 | 0 | 0 | 0 | 1 | 0 | 0 | size | 0 | Zm | 0 | 1 | 1 | 1 | 0 | 0 | Zn | Zda
|  |  |  |  | S |  |

####

SQRDMLAH <Zda>.<T>, <Zn>.<T>, <Zm>.<T>

if !HaveSVE2() && !HaveSME() then UNDEFINED; constant integer esize = 8 << UInt(size); integer n = UInt(Zn); integer m = UInt(Zm); integer da = UInt(Zda);

### Assembler Symbols

<Zda> | Is the name of the third source and destination scalable vector register, encoded in the "Zda" field.

<T> | Is the size specifier, encoded in size:
size | <T>
--- | ---
00 | B
01 | H
10 | S
11 | D

<Zn> | Is the name of the first source scalable vector register, encoded in the "Zn" field.

<Zm> | Is the name of the second source scalable vector register, encoded in the "Zm" field.

### Operation

CheckSVEEnabled(); constant integer VL = CurrentVL; constant integer elements = VL DIV esize; bits(VL) operand1 = Z[n, VL]; bits(VL) operand2 = Z[m, VL]; bits(VL) operand3 = Z[da, VL]; bits(VL) result; constant integer round_const = 1 << (esize - 1); for e = 0 to elements-1 integer element1 = SInt(Elem[operand1, e, esize]); integer element2 = SInt(Elem[operand2, e, esize]); integer element3 = SInt(Elem[operand3, e, esize]); integer res = (element3 << esize) + (2 * element1 * element2); Elem[result, e, esize] = SignedSat((res + round_const) >> esize, esize); Z[da, VL] = result;

### Operational information

If FEAT_SVE2 is implemented or FEAT_SME is implemented, then when PSTATE.DIT is 1:

- The execution time of this instruction is independent of:
  - The values of the data supplied in any of its registers.
  - The values of the NZCV flags.
- The response of this instruction to asynchronous exceptions does not vary based on:
  - The values of the data supplied in any of its registers.
  - The values of the NZCV flags.

This instruction might be immediately preceded in program order by a MOVPRFX instruction. The MOVPRFX instruction must conform to all of the following requirements, otherwise the behavior of the MOVPRFX and this instruction is unpredictable:

- The MOVPRFX instruction must be unpredicated.
- The MOVPRFX instruction must specify the same destination register as this instruction.
- The destination register must not refer to architectural register state referenced by any other source operand register of this instruction.

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: isa v33.53, AdvSIMD v29.11, pseudocode v2022-09_rel, sve v2022-09_rel ; Build timestamp: 2022-09-30T16:37

Copyright © 2010-2022 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.