Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## CLASTB (vectors)

Conditionally extract last element to vector register

From the second source vector register extract the last active element, and then replicate that element to destructively fill the destination and first source vector.

If there are no active elements then leave the destination and source vector unmodified.

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | 0 | 0 | 0 | 0 | 1 | 0 | 1 | size | 1 | 0 | 1 | 0 | 0 | 1 | 1 | 0 | 0 | Pg | Zm | Zdn
|  |  | B |  |  |  |

####

CLASTB <Zdn>.<T>, <Pg>, <Zdn>.<T>, <Zm>.<T>

if !HaveSVE() && !HaveSME() then UNDEFINED; constant integer esize = 8 << UInt(size); integer g = UInt(Pg); integer dn = UInt(Zdn); integer m = UInt(Zm); boolean isBefore = TRUE;

### Assembler Symbols

<Zdn> | Is the name of the first source and destination scalable vector register, encoded in the "Zdn" field.

<T> | Is the size specifier, encoded in size:
size | <T>
--- | ---
00 | B
01 | H
10 | S
11 | D

<Pg> | Is the name of the governing scalable predicate register P0-P7, encoded in the "Pg" field.

<Zm> | Is the name of the second source scalable vector register, encoded in the "Zm" field.

### Operation

CheckSVEEnabled(); constant integer VL = CurrentVL; constant integer PL = VL DIV 8; constant integer elements = VL DIV esize; bits(PL) mask = P[g, PL]; bits(VL) operand1 = Z[dn, VL]; bits(VL) operand2 = Z[m, VL]; bits(VL) result; integer last = LastActiveElement(mask, esize); if last < 0 then result = operand1; else if !isBefore then last = last + 1; if last >= elements then last = 0; for e = 0 to elements-1 Elem[result, e, esize] = Elem[operand2, last, esize]; Z[dn, VL] = result;

### Operational information

This instruction might be immediately preceded in program order by a MOVPRFX instruction. The MOVPRFX instruction must conform to all of the following requirements, otherwise the behavior of the MOVPRFX and this instruction is unpredictable:

- The MOVPRFX instruction must be unpredicated.
- The MOVPRFX instruction must specify the same destination register as this instruction.
- The destination register must not refer to architectural register state referenced by any other source operand register of this instruction.

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: isa v33.53, AdvSIMD v29.11, pseudocode v2022-09_rel, sve v2022-09_rel ; Build timestamp: 2022-09-30T16:37

Copyright © 2010-2022 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.