AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# HACTLR2, Hyp Auxiliary Control Register 2

The HACTLR2 characteristics are:

## Purpose

Provides additional space to the HACTLR register to hold IMPLEMENTATION DEFINED trap functionality.

## Configuration

AArch32 System register HACTLR2 bits [31:0] are architecturally mapped to AArch64 System register ACTLR_EL2[63:32].

This register is present only when EL2 is capable of using AArch32. Otherwise, direct accesses to HACTLR2 are UNDEFINED.

In Armv8.0 and Armv8.1, it is IMPLEMENTATION DEFINED whether this register is implemented, or whether it causes UNDEFINED exceptions when accessed. The implementation of this register can be detected by examining ID_MMFR4.AC2.

From Armv8.2 this register must be implemented.

## Attributes

HACTLR2 is a 32-bit register.

## Field descriptions

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
IMPLEMENTATION DEFINED

#### IMPLEMENTATION DEFINED, bits [31:0]

IMPLEMENTATION DEFINED.

The reset behavior of this field is:

- On a Warm reset, this field resets to an architecturally UNKNOWN value.

## Accessing HACTLR2

Accesses to this register use the following encodings in the System register encoding space:

#### MRC{<c>}{<q>} <coproc>, {#}<opc1>, <Rt>, <CRn>, <CRm>{, {#}<opc2>}

coproc | opc1 | CRn | CRm | opc2
--- | --- | --- | --- | ---
0b1111 | 0b100 | 0b0001 | 0b0000 | 0b011

if PSTATE.EL == EL0 then UNDEFINED; elsif PSTATE.EL == EL1 then if EL2Enabled() && !ELUsingAArch32(EL2) && HSTR_EL2.T1 == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HSTR.T1 == '1' then AArch32.TakeHypTrapException(0x03); else UNDEFINED; elsif PSTATE.EL == EL2 then R[t] = HACTLR2; elsif PSTATE.EL == EL3 then if SCR.NS == '0' then UNDEFINED; else R[t] = HACTLR2;

#### MCR{<c>}{<q>} <coproc>, {#}<opc1>, <Rt>, <CRn>, <CRm>{, {#}<opc2>}

coproc | opc1 | CRn | CRm | opc2
--- | --- | --- | --- | ---
0b1111 | 0b100 | 0b0001 | 0b0000 | 0b011

if PSTATE.EL == EL0 then UNDEFINED; elsif PSTATE.EL == EL1 then if EL2Enabled() && !ELUsingAArch32(EL2) && HSTR_EL2.T1 == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HSTR.T1 == '1' then AArch32.TakeHypTrapException(0x03); else UNDEFINED; elsif PSTATE.EL == EL2 then HACTLR2 = R[t]; elsif PSTATE.EL == EL3 then if SCR.NS == '0' then UNDEFINED; else HACTLR2 = R[t];

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.