Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## FACLE

Floating-point absolute compare less than or equal

Compare active absolute values of floating-point elements in the first source vector being less than or equal to corresponding absolute values of elements in the second source vector, and place the boolean results of the comparison in the corresponding elements of the destination predicate. Inactive elements in the destination predicate register are set to zero. Does not set the condition flags.

This is a pseudo-instruction of FAC<cc>. This means:

- The encodings in this description are named to match the encodings of FAC<cc>.
- The assembler syntax is used only for assembly, and is not used on disassembly.
- The description of FAC<cc> gives the operational pseudocode for this instruction.

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | 1 | 1 | 0 | 0 | 1 | 0 | 1 | size | 0 | Zm | 1 | 1 | 0 | Pg | Zn | 1 | Pd

####

FACLE <Pd>.<T>, <Pg>/Z, <Zm>.<T>, <Zn>.<T>

is equivalent to

FACGE <Pd>.<T>, <Pg>/Z, <Zn>.<T>, <Zm>.<T>

### Assembler Symbols

<Pd> | Is the name of the destination scalable predicate register, encoded in the "Pd" field.

<Zm> | Is the name of the second source scalable vector register, encoded in the "Zm" field.

<Zn> | Is the name of the first source scalable vector register, encoded in the "Zn" field.

<T> | Is the size specifier, encoded in size:
size | <T>
--- | ---
00 | RESERVED
01 | H
10 | S
11 | D

<Pg> | Is the name of the governing scalable predicate register P0-P7, encoded in the "Pg" field.

### Operation

The description of FAC<cc> gives the operational pseudocode for this instruction.

### Operational information

If FEAT_SME is implemented and the PE is in Streaming SVE mode, then any subsequent instruction which is dependent on the predicate register written by this instruction might be significantly delayed.

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: isa v33.53, AdvSIMD v29.11, pseudocode v2022-09_rel, sve v2022-09_rel ; Build timestamp: 2022-09-30T16:37

Copyright © 2010-2022 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.