Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## FCVTZU (vector, integer)

Floating-point Convert to Unsigned integer, rounding toward Zero (vector). This instruction converts a scalar or each element in a vector from a floating-point value to an unsigned integer value using the Round towards Zero rounding mode, and writes the result to the SIMD&FP destination register.

A floating-point exception can be generated by this instruction. Depending on the settings in FPCR, the exception results in either a flag being set in FPSR, or a synchronous exception being generated. For more information, see Floating-point exception traps.

Depending on the settings in the CPACR_EL1, CPTR_EL2, and CPTR_EL3 registers, and the Security state and Exception level in which the instruction is executed, an attempt to execute the instruction might be trapped.

It has encodings from 4 classes: Scalar half precision , Scalar single-precision and double-precision , Vector half precision and Vector single-precision and double-precision

### Scalar half precision
(FEAT_FP16)

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | 1 | 1 | 1 | 1 | 1 | 1 | 0 | 1 | 1 | 1 | 1 | 1 | 0 | 0 | 1 | 1 | 0 | 1 | 1 | 1 | 0 | Rn | Rd
| U |  | o2 |  |  | o1 |  |  |

####

FCVTZU <Hd>, <Hn>

if !HaveFP16Ext() then UNDEFINED; integer d = UInt(Rd); integer n = UInt(Rn); integer esize = 16; integer datasize = esize; integer elements = 1; FPRounding rounding = FPDecodeRounding(o1:o2); boolean unsigned = (U == '1');

### Scalar single-precision and double-precision

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | 1 | 1 | 1 | 1 | 1 | 1 | 0 | 1 | sz | 1 | 0 | 0 | 0 | 0 | 1 | 1 | 0 | 1 | 1 | 1 | 0 | Rn | Rd
| U |  | o2 |  |  |  | o1 |  |  |

####

FCVTZU <V><d>, <V><n>

integer d = UInt(Rd); integer n = UInt(Rn); integer esize = 32 << UInt(sz); integer datasize = esize; integer elements = 1; FPRounding rounding = FPDecodeRounding(o1:o2); boolean unsigned = (U == '1');

### Vector half precision
(FEAT_FP16)

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | Q | 1 | 0 | 1 | 1 | 1 | 0 | 1 | 1 | 1 | 1 | 1 | 0 | 0 | 1 | 1 | 0 | 1 | 1 | 1 | 0 | Rn | Rd
|  | U |  | o2 |  |  | o1 |  |  |

####

FCVTZU <Vd>.<T>, <Vn>.<T>

if !HaveFP16Ext() then UNDEFINED; integer d = UInt(Rd); integer n = UInt(Rn); integer esize = 16; integer datasize = if Q == '1' then 128 else 64; integer elements = datasize DIV esize; FPRounding rounding = FPDecodeRounding(o1:o2); boolean unsigned = (U == '1');

### Vector single-precision and double-precision

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | Q | 1 | 0 | 1 | 1 | 1 | 0 | 1 | sz | 1 | 0 | 0 | 0 | 0 | 1 | 1 | 0 | 1 | 1 | 1 | 0 | Rn | Rd
|  | U |  | o2 |  |  |  | o1 |  |  |

####

FCVTZU <Vd>.<T>, <Vn>.<T>

integer d = UInt(Rd); integer n = UInt(Rn); if sz:Q == '10' then UNDEFINED; integer esize = 32 << UInt(sz); integer datasize = if Q == '1' then 128 else 64; integer elements = datasize DIV esize; FPRounding rounding = FPDecodeRounding(o1:o2); boolean unsigned = (U == '1');

### Assembler Symbols

<Hd> | Is the 16-bit name of the SIMD&FP destination register, encoded in the "Rd" field.

<Hn> | Is the 16-bit name of the SIMD&FP source register, encoded in the "Rn" field.

<V> | Is a width specifier, encoded in sz:
sz | <V>
--- | ---
0 | S
1 | D

<d> | Is the number of the SIMD&FP destination register, encoded in the "Rd" field.

<n> | Is the number of the SIMD&FP source register, encoded in the "Rn" field.

<Vd> | Is the name of the SIMD&FP destination register, encoded in the "Rd" field.

<T> | For the half-precision variant: is an arrangement specifier, encoded in Q:
Q | <T>
--- | ---
0 | 4H
1 | 8H
| For the single-precision and double-precision variant: is an arrangement specifier, encoded in sz:Q:
sz | Q | <T>
--- | --- | ---
0 | 0 | 2S
0 | 1 | 4S
1 | 0 | RESERVED
1 | 1 | 2D

<Vn> | Is the name of the SIMD&FP source register, encoded in the "Rn" field.

### Operation

CheckFPAdvSIMDEnabled64(); bits(datasize) operand = V[n, datasize]; bits(esize) element; FPCRType fpcr = FPCR[]; boolean merge = elements == 1 && IsMerging(fpcr); bits(128) result = if merge then V[d, 128] else Zeros(128); for e = 0 to elements-1 element = Elem[operand, e, esize]; Elem[result, e, esize] = FPToFixed(element, 0, unsigned, fpcr, rounding, esize); V[d, 128] = result;

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: isa v33.64, AdvSIMD v29.12, pseudocode v2023-06_rel, sve v2023-06_rel ; Build timestamp: 2023-07-04T19:42

Copyright © 2010-2023 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.