Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## SQRDMLSH (vectors)

Signed saturating rounding doubling multiply-subtract high from accumulator (unpredicated)

Multiply then double the corresponding signed elements of the first and second source vectors, and destructively subtract the rounded high half of each result from the corresponding elements of the addend and destination vector. Each destination element is saturated to the N-bit element's signed integer range -2(N-1) to (2(N-1) )-1. This instruction is unpredicated.

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | 1 | 0 | 0 | 0 | 1 | 0 | 0 | size | 0 | Zm | 0 | 1 | 1 | 1 | 0 | 1 | Zn | Zda
|  |  |  |  | S |  |

####

SQRDMLSH <Zda>.<T>, <Zn>.<T>, <Zm>.<T>

if !HaveSVE2() && !HaveSME() then UNDEFINED; constant integer esize = 8 << UInt(size); integer n = UInt(Zn); integer m = UInt(Zm); integer da = UInt(Zda);

### Assembler Symbols

<Zda> | Is the name of the third source and destination scalable vector register, encoded in the "Zda" field.

<T> | Is the size specifier, encoded in size:
size | <T>
--- | ---
00 | B
01 | H
10 | S
11 | D

<Zn> | Is the name of the first source scalable vector register, encoded in the "Zn" field.

<Zm> | Is the name of the second source scalable vector register, encoded in the "Zm" field.

### Operation

CheckSVEEnabled(); constant integer VL = CurrentVL; constant integer elements = VL DIV esize; bits(VL) operand1 = Z[n, VL]; bits(VL) operand2 = Z[m, VL]; bits(VL) operand3 = Z[da, VL]; bits(VL) result; for e = 0 to elements-1 integer element1 = SInt(Elem[operand1, e, esize]); integer element2 = SInt(Elem[operand2, e, esize]); integer element3 = SInt(Elem[operand3, e, esize]); integer res = (element3 << esize) - (2 * element1 * element2); Elem[result, e, esize] = SignedSat((res + (1 << (esize - 1))) >> esize, esize); Z[da, VL] = result;

### Operational information

This instruction might be immediately preceded in program order by a MOVPRFX instruction. The MOVPRFX instruction must conform to all of the following requirements, otherwise the behavior of the MOVPRFX and this instruction is unpredictable:

- The MOVPRFX instruction must be unpredicated.
- The MOVPRFX instruction must specify the same destination register as this instruction.
- The destination register must not refer to architectural register state referenced by any other source operand register of this instruction.

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: isa v33.64, AdvSIMD v29.12, pseudocode v2023-06_rel, sve v2023-06_rel ; Build timestamp: 2023-07-04T19:42

Copyright © 2010-2023 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.