AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# AMEVTYPER1<n>, Activity Monitors Event Type Registers 1, n = 0 - 15

The AMEVTYPER1<n> characteristics are:

## Purpose

Provides information on the events that an auxiliary activity monitor event counter AMEVCNTR1<n> counts.

## Configuration

AArch32 System register AMEVTYPER1<n> bits [31:0] are architecturally mapped to AArch64 System register AMEVTYPER1<n>_EL0[31:0].

AArch32 System register AMEVTYPER1<n> bits [31:0] are architecturally mapped to External register AMU.AMEVTYPER1<n>[31:0].

This register is present only when FEAT_AMUv1 is implemented and AArch32 is supported. Otherwise, direct accesses to AMEVTYPER1<n> are UNDEFINED.

## Attributes

AMEVTYPER1<n> is a 32-bit register.

## Field descriptions

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
RES0 | evtCount

#### Bits [31:16]

Reserved, RES0.

#### evtCount, bits [15:0]

Event to count. The event number of the event that is counted by the auxiliary activity monitor event counter AMEVCNTR1<n>.

It is IMPLEMENTATION DEFINED what values are supported by each counter.

If software writes a value to this field which is not supported by the corresponding counter AMEVCNTR1<n>, then:

- It is UNPREDICTABLE which event will be counted.
- The value read back is UNKNOWN.

The event counted by AMEVCNTR1<n> might be fixed at implementation. In this case, the field is read-only and writes are UNDEFINED.

If the corresponding counter AMEVCNTR1<n> is enabled, writes to this register have UNPREDICTABLE results.

The reset behavior of this field is:

- On a Warm reset, this field resets to an architecturally UNKNOWN value.

## Accessing AMEVTYPER1<n>

If <n> is greater than or equal to the number of auxiliary activity monitor event counters, reads and writes of AMEVTYPER1<n> are UNDEFINED.

Note

AMCGCR.CG1NC identifies the number of auxiliary activity monitor event counters.

Accesses to this register use the following encodings in the System register encoding space:

#### MRC{<c>}{<q>} <coproc>, {#}<opc1>, <Rt>, <CRn>, <CRm>{, {#}<opc2>} ; Where m = 0-15

coproc | opc1 | CRn | CRm | opc2
--- | --- | --- | --- | ---
0b1111 | 0b000 | 0b1101 | 0b111:m[3] | m[2:0]

integer m = UInt(CRm<0>:opc2<2:0>); if m >= NUM_AMU_CG1_MONITORS then UNDEFINED; elsif !IsG1ActivityMonitorImplemented(m) then UNDEFINED; elsif PSTATE.EL == EL0 then if HaveEL(EL3) && EL3SDDUndefPriority() && !ELUsingAArch32(EL3) && CPTR_EL3.TAM == '1' then UNDEFINED; elsif !ELUsingAArch32(EL1) && AMUSERENR_EL0.EN == '0' then if EL2Enabled() && !ELUsingAArch32(EL2) && HCR_EL2.TGE == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); else AArch64.AArch32SystemAccessTrap(EL1, 0x03); elsif ELUsingAArch32(EL1) && AMUSERENR.EN == '0' then if EL2Enabled() && !ELUsingAArch32(EL2) && HCR_EL2.TGE == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HCR.TGE == '1' then AArch32.TakeHypTrapException(0x00); else UNDEFINED; elsif EL2Enabled() && !ELUsingAArch32(EL2) && !ELIsInHost(EL0) && HSTR_EL2.T13 == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HSTR.T13 == '1' then AArch32.TakeHypTrapException(0x03); elsif EL2Enabled() && !ELUsingAArch32(EL2) && CPTR_EL2.TAM == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HCPTR.TAM == '1' then AArch32.TakeHypTrapException(0x03); elsif EL2Enabled() && !ELUsingAArch32(EL1) && !ELIsInHost(EL0) && IsFeatureImplemented(FEAT_FGT) && (!HaveEL(EL3) || SCR_EL3.FGTEn == '1') && HAFGRTR_EL2.AMEVTYPER1<m>_EL0 == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif HaveEL(EL3) && !ELUsingAArch32(EL3) && CPTR_EL3.TAM == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.AArch32SystemAccessTrap(EL3, 0x03); else R[t] = AMEVTYPER1[m]; elsif PSTATE.EL == EL1 then if HaveEL(EL3) && EL3SDDUndefPriority() && !ELUsingAArch32(EL3) && CPTR_EL3.TAM == '1' then UNDEFINED; elsif EL2Enabled() && !ELUsingAArch32(EL2) && HSTR_EL2.T13 == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HSTR.T13 == '1' then AArch32.TakeHypTrapException(0x03); elsif EL2Enabled() && !ELUsingAArch32(EL2) && CPTR_EL2.TAM == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HCPTR.TAM == '1' then AArch32.TakeHypTrapException(0x03); elsif HaveEL(EL3) && !ELUsingAArch32(EL3) && CPTR_EL3.TAM == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.AArch32SystemAccessTrap(EL3, 0x03); else R[t] = AMEVTYPER1[m]; elsif PSTATE.EL == EL2 then if HaveEL(EL3) && EL3SDDUndefPriority() && !ELUsingAArch32(EL3) && CPTR_EL3.TAM == '1' then UNDEFINED; elsif HaveEL(EL3) && !ELUsingAArch32(EL3) && CPTR_EL3.TAM == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.AArch32SystemAccessTrap(EL3, 0x03); else R[t] = AMEVTYPER1[m]; elsif PSTATE.EL == EL3 then R[t] = AMEVTYPER1[m];

#### MCR{<c>}{<q>} <coproc>, {#}<opc1>, <Rt>, <CRn>, <CRm>{, {#}<opc2>} ; Where m = 0-15

coproc | opc1 | CRn | CRm | opc2
--- | --- | --- | --- | ---
0b1111 | 0b000 | 0b1101 | 0b111:m[3] | m[2:0]

integer m = UInt(CRm<0>:opc2<2:0>); if m >= NUM_AMU_CG1_MONITORS then UNDEFINED; elsif !IsG1ActivityMonitorImplemented(m) then UNDEFINED; elsif PSTATE.EL == EL1 && EL2Enabled() && !ELUsingAArch32(EL2) && HSTR_EL2.T13 == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif PSTATE.EL == EL1 && EL2Enabled() && ELUsingAArch32(EL2) && HSTR.T13 == '1' then AArch32.TakeHypTrapException(0x03); elsif IsHighestEL(PSTATE.EL) && !boolean IMPLEMENTATION_DEFINED "AMEVCNTR1[m] is fixed" then AMEVTYPER1[m] = R[t]; else UNDEFINED;

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.