Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## LDAPRH

Load-Acquire RCpc Register Halfword derives an address from a base register value, loads a halfword from the derived address in memory, zero-extends it and writes it to a register.

The instruction has memory ordering semantics as described in Load-Acquire, Load-AcquirePC, and Store-Release, except that:

- There is no ordering requirement, separate from the requirements of a Load-AcquirePC or a Store-Release, created by having a Store-Release followed by a Load-AcquirePC instruction.
- The reading of a value written by a Store-Release by a Load-AcquirePC instruction by the same observer does not make the write of the Store-Release globally observed.

This difference in memory ordering is not described in the pseudocode.

For information about memory accesses, see Load/Store addressing modes.

### Integer
(FEAT_LRCPC)

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | 1 | 1 | 1 | 1 | 0 | 0 | 0 | 1 | 0 | 1 | (1) | (1) | (1) | (1) | (1) | 1 | 1 | 0 | 0 | 0 | 0 | Rn | Rt
size |  |  |  |  |  |  | Rs |  |  |  |  |

####

LDAPRH <Wt>, [<Xn|SP> {,#0}]

integer n = UInt(Rn); integer t = UInt(Rt); boolean tagchecked = n != 31;

### Assembler Symbols

<Wt> | Is the 32-bit name of the general-purpose register to be loaded, encoded in the "Rt" field.

<Xn|SP> | Is the 64-bit name of the general-purpose base register or stack pointer, encoded in the "Rn" field.

### Operation

bits(64) address; bits(16) data; AccessDescriptor accdesc = CreateAccDescLDAcqPC(tagchecked); if n == 31 then CheckSPAlignment(); address = SP[]; else address = X[n, 64]; data = Mem[address, 2, accdesc]; X[t, 32] = ZeroExtend(data, 32);

### Operational information

If PSTATE.DIT is 1, the timing of this instruction is insensitive to the value of the data being loaded or stored.

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: isa v33.74, AdvSIMD v29.23, pseudocode v2023-09_rel, sve v2023-09_rc3 ; Build timestamp: 2023-09-27T17:06

Copyright © 2010-2023 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.