Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## LD1Q

Gather load quadwords

Gather load of quadwords to active elements of a vector register from memory addresses generated by a vector base plus a 64-bit unscaled scalar register offset. Inactive elements will not cause a read from Device memory or signal faults, and are set to zero in the destination vector.

This instruction is illegal when executed in Streaming SVE mode, unless FEAT_SME_FA64 is implemented and enabled.

### SVE2
(FEAT_SVE2p1)

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
1 | 1 | 0 | 0 | 0 | 1 | 0 | 0 | 0 | 0 | 0 | Rm | 1 | 0 | 1 | Pg | Zn | Zt

####

LD1Q { <Zt>.Q }, <Pg>/Z, [<Zn>.D{, <Xm>}]

if !IsFeatureImplemented(FEAT_SVE2p1) then UNDEFINED; constant integer t = UInt(Zt); constant integer n = UInt(Zn); constant integer m = UInt(Rm); constant integer g = UInt(Pg);

### Assembler Symbols

<Zt> | Is the name of the scalable vector register to be transferred, encoded in the "Zt" field.

<Pg> | Is the name of the governing scalable predicate register P0-P7, encoded in the "Pg" field.

<Zn> | Is the name of the base scalable vector register, encoded in the "Zn" field.

<Xm> | Is the optional 64-bit name of the general-purpose offset register, defaulting to XZR, encoded in the "Rm" field.

### Operation

constant integer VL = CurrentVL; constant integer PL = VL DIV 8; CheckNonStreamingSVEEnabled(); constant integer elements = VL DIV 128; constant bits(PL) mask = P[g, PL]; bits(VL) base; bits(64) offset; bits(VL) result; constant boolean contiguous = FALSE; constant boolean nontemporal = FALSE; constant boolean tagchecked = TRUE; constant AccessDescriptor accdesc = CreateAccDescSVE(MemOp_LOAD, nontemporal, contiguous, tagchecked); if AnyActiveElement(mask, 128) then base = Z[n, VL]; offset = X[m, 64]; for e = 0 to elements-1 if ActivePredicateElement(mask, e, 128) then constant bits(64) baddr = Elem[base, 2*e, 64]; constant bits(64) addr = AddressAdd(baddr, offset, accdesc); Elem[result, e, 128] = Mem[addr, 16, accdesc]; else Elem[result, e, 128] = Zeros(128); Z[t, VL] = result;

### Operational information

If PSTATE.DIT is 1, the timing of this instruction is insensitive to the value of the data being loaded or stored when its governing predicate register contains the same value for each execution.

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: aarchmrs v2024-03_relA, pseudocode v2024-03_rel, sve v2024-03_rel ; Build timestamp: 2024-03-26T09:45

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.