Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## UZP2

Unzip vectors (secondary). This instruction reads corresponding odd-numbered vector elements from the two source SIMD&FP registers, places the result from the first source register into consecutive elements in the lower half of a vector, and the result from the second source register into consecutive elements in the upper half of a vector, and writes the vector to the destination SIMD&FP register.

#### Note

This instruction can be used with UZP1 to de-interleave two vectors.

The following figure shows an example of the operation of UZP1 and UZP2 with the arrangement specifier 8B.

Depending on the settings in the CPACR_EL1, CPTR_EL2, and CPTR_EL3 registers, and the current Security state and Exception level, an attempt to execute the instruction might be trapped.

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | Q | 0 | 0 | 1 | 1 | 1 | 0 | size | 0 | Rm | 0 | 1 | 0 | 1 | 1 | 0 | Rn | Rd
|  |  |  |  |  |  | op |  |  |  |

####

UZP2 <Vd>.<T>, <Vn>.<T>, <Vm>.<T>

integer d = UInt(Rd); integer n = UInt(Rn); integer m = UInt(Rm); if size:Q == '110' then UNDEFINED; constant integer esize = 8 << UInt(size); constant integer datasize = 64 << UInt(Q); integer elements = datasize DIV esize; integer part = UInt(op);

### Assembler Symbols

<Vd> | Is the name of the SIMD&FP destination register, encoded in the "Rd" field.

<T> | Is an arrangement specifier, encoded in size:Q:
size | Q | <T>
--- | --- | ---
00 | 0 | 8B
00 | 1 | 16B
01 | 0 | 4H
01 | 1 | 8H
10 | 0 | 2S
10 | 1 | 4S
11 | 0 | RESERVED
11 | 1 | 2D

<Vn> | Is the name of the first SIMD&FP source register, encoded in the "Rn" field.

<Vm> | Is the name of the second SIMD&FP source register, encoded in the "Rm" field.

### Operation

CheckFPAdvSIMDEnabled64(); bits(datasize) operandl = V[n, datasize]; bits(datasize) operandh = V[m, datasize]; bits(datasize) result; bits(datasize*2) zipped = operandh:operandl; for e = 0 to elements-1 Elem[result, e, esize] = Elem[zipped, 2*e+part, esize]; V[d, datasize] = result;

### Operational information

If PSTATE.DIT is 1:

- The execution time of this instruction is independent of:
  - The values of the data supplied in any of its registers.
  - The values of the NZCV flags.
- The response of this instruction to asynchronous exceptions does not vary based on:
  - The values of the data supplied in any of its registers.
  - The values of the NZCV flags.

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: isa v33.74, AdvSIMD v29.23, pseudocode v2023-09_rel, sve v2023-09_rc3 ; Build timestamp: 2023-09-27T17:06

Copyright © 2010-2023 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.