AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# GICD_IGRPMODR<n>E, Interrupt Group Modifier Registers (extended SPI range), n = 0 - 31

The GICD_IGRPMODR<n>E characteristics are:

## Purpose

When GICD_CTLR.DS==0, this register together with the GICD_IGROUPR<n>E registers, controls whether the corresponding interrupt is in:

- Secure Group 0.
- Non-secure Group 1.
- When System register access is enabled, Secure Group 1.

## Configuration

This register is present only when GICv3.1 is implemented. Otherwise, direct accesses to GICD_IGRPMODR<n>E are RES0.

GICD_IGRPMODR<n>E resets to 0x00000000.

When GICD_TYPER.ESPI==0, these registers are RES0.

When GICD_TYPER.ESPI==1:

- The number of implemented GICD_IGRPMODR<n>E registers is (GICD_TYPER.ESPI_range+1). Registers are numbered from 0.
- When GICD_CTLR.DS==0, this register is Secure.

## Attributes

GICD_IGRPMODR<n>E is a 32-bit register.

## Field descriptions

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
Group_modifier_bit31 | Group_modifier_bit30 | Group_modifier_bit29 | Group_modifier_bit28 | Group_modifier_bit27 | Group_modifier_bit26 | Group_modifier_bit25 | Group_modifier_bit24 | Group_modifier_bit23 | Group_modifier_bit22 | Group_modifier_bit21 | Group_modifier_bit20 | Group_modifier_bit19 | Group_modifier_bit18 | Group_modifier_bit17 | Group_modifier_bit16 | Group_modifier_bit15 | Group_modifier_bit14 | Group_modifier_bit13 | Group_modifier_bit12 | Group_modifier_bit11 | Group_modifier_bit10 | Group_modifier_bit9 | Group_modifier_bit8 | Group_modifier_bit7 | Group_modifier_bit6 | Group_modifier_bit5 | Group_modifier_bit4 | Group_modifier_bit3 | Group_modifier_bit2 | Group_modifier_bit1 | Group_modifier_bit0

#### Group_modifier_bit<x>, bit [x], for x = 31 to 0

Group modifier bit. In implementations where affinity routing is enabled for the Security state of an interrupt, the bit that corresponds to the interrupt is concatenated with the equivalent bit in GICD_IGROUPR<n>E to form a 2-bit field that defines an interrupt group:

Group modifier bit | Group status bit | Definition | Short name
--- | --- | --- | ---
0b0 | 0b0 | Secure Group 0 | G0S
0b0 | 0b1 | Non-secure Group 1 | G1NS
0b1 | 0b0 | Secure Group 1 | G1S
0b1 | 0b1 | Reserved, treated as Non-secure Group 1 | -

The reset behavior of this field is:

- On a GIC reset, this field resets to 0.

#### Additional information

For INTID m, when DIV and MOD are the integer division and modulo operations:

- The corresponding GICD_IGRPMODR<n>E number, n, is given by n = (m-4096) DIV 32.
- The offset of the required GICD_IGRPMODR<n>E is (0x3400 + (4*n)).
- The bit number of the required group modifier bit in this register is (m-4096) MOD 32.

## Accessing GICD_IGRPMODR<n>E

When affinity routing is not enabled for the Security state of an interrupt in GICD_IGRPMODR<n>E, the corresponding bit is RES0.

When GICD_CTLR.DS==0, bits corresponding to Secure SPIs are RAZ/WI to Non-secure accesses.

Bits corresponding to unimplemented interrupts are RAZ/WI.

#### GICD_IGRPMODR<n>E can be accessed through the memory-mapped interfaces:

Component | Frame | Offset | Instance
--- | --- | --- | ---
GIC Distributor | Dist_base | 0x3400 + (4 * n) | GICD_IGRPMODR<n>E

Accesses on this interface are RW.

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.