AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# DBGDCCINT, DCC Interrupt Enable Register

The DBGDCCINT characteristics are:

## Purpose

Enables interrupt requests to be signaled based on the DCC status flags.

## Configuration

AArch32 System register DBGDCCINT bits [31:0] are architecturally mapped to AArch64 System register MDCCINT_EL1[31:0].

This register is present only when EL1 is capable of using AArch32. Otherwise, direct accesses to DBGDCCINT are UNDEFINED.

## Attributes

DBGDCCINT is a 32-bit register.

## Field descriptions

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
RES0 | RX | TX | RES0

#### Bit [31]

Reserved, RES0.

#### RX, bit [30]

DCC interrupt request enable control for DTRRX. Enables a common COMMIRQ interrupt request to be signaled based on the DCC status flags.

RX | Meaning
--- | ---
0b0 | No interrupt request generated by DTRRX.
0b1 | Interrupt request will be generated on RXfull == 1.

If legacy COMMRX and COMMTX signals are implemented, then these are not affected by the value of this bit.

The reset behavior of this field is:

- On a Warm reset, this field resets to 0.

#### TX, bit [29]

DCC interrupt request enable control for DTRTX. Enables a common COMMIRQ interrupt request to be signaled based on the DCC status flags.

TX | Meaning
--- | ---
0b0 | No interrupt request generated by DTRTX.
0b1 | Interrupt request will be generated on TXfull == 0.

If legacy COMMRX and COMMTX signals are implemented, then these are not affected by the value of this bit.

The reset behavior of this field is:

- On a Warm reset, this field resets to 0.

#### Bits [28:0]

Reserved, RES0.

## Accessing DBGDCCINT

Accesses to this register use the following encodings in the System register encoding space:

#### MRC{<c>}{<q>} <coproc>, {#}<opc1>, <Rt>, <CRn>, <CRm>{, {#}<opc2>}

coproc | opc1 | CRn | CRm | opc2
--- | --- | --- | --- | ---
0b1110 | 0b000 | 0b0000 | 0b0010 | 0b000

if PSTATE.EL == EL0 then UNDEFINED; elsif Halted() && ConstrainUnpredictableBool(Unpredictable_IGNORETRAPINDEBUG) then R[t] = DBGDCCINT; elsif PSTATE.EL == EL1 then if HaveEL(EL3) && EL3SDDUndefPriority() && !ELUsingAArch32(EL3) && IsFeatureImplemented(FEAT_FGT) && MDCR_EL3.TDCC == '1' then UNDEFINED; elsif HaveEL(EL3) && EL3SDDUndefPriority() && ELUsingAArch32(EL3) && SDCR.TDCC == '1' then UNDEFINED; elsif HaveEL(EL3) && EL3SDDUndefPriority() && !ELUsingAArch32(EL3) && MDCR_EL3.TDA == '1' then UNDEFINED; elsif EL2Enabled() && !ELUsingAArch32(EL2) && IsFeatureImplemented(FEAT_FGT) && MDCR_EL2.TDCC == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x05); elsif EL2Enabled() && ELUsingAArch32(EL2) && HDCR.TDCC == '1' then AArch32.TakeHypTrapException(0x05); elsif EL2Enabled() && !ELUsingAArch32(EL2) && MDCR_EL2.<TDE,TDA> != '00' then AArch64.AArch32SystemAccessTrap(EL2, 0x05); elsif EL2Enabled() && ELUsingAArch32(EL2) && HDCR.<TDE,TDA> != '00' then AArch32.TakeHypTrapException(0x05); elsif HaveEL(EL3) && !ELUsingAArch32(EL3) && IsFeatureImplemented(FEAT_FGT) && MDCR_EL3.TDCC == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.AArch32SystemAccessTrap(EL3, 0x05); elsif HaveEL(EL3) && ELUsingAArch32(EL3) && SDCR.TDCC == '1' then if EL3SDDUndef() then UNDEFINED; else AArch32.TakeMonitorTrapException(); elsif HaveEL(EL3) && !ELUsingAArch32(EL3) && MDCR_EL3.TDA == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.AArch32SystemAccessTrap(EL3, 0x05); else R[t] = DBGDCCINT; elsif PSTATE.EL == EL2 then if HaveEL(EL3) && EL3SDDUndefPriority() && !ELUsingAArch32(EL3) && IsFeatureImplemented(FEAT_FGT) && MDCR_EL3.TDCC == '1' then UNDEFINED; elsif HaveEL(EL3) && EL3SDDUndefPriority() && ELUsingAArch32(EL3) && SDCR.TDCC == '1' then UNDEFINED; elsif HaveEL(EL3) && EL3SDDUndefPriority() && !ELUsingAArch32(EL3) && MDCR_EL3.TDA == '1' then UNDEFINED; elsif HaveEL(EL3) && !ELUsingAArch32(EL3) && IsFeatureImplemented(FEAT_FGT) && MDCR_EL3.TDCC == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.AArch32SystemAccessTrap(EL3, 0x05); elsif HaveEL(EL3) && ELUsingAArch32(EL3) && SDCR.TDCC == '1' then if EL3SDDUndef() then UNDEFINED; else AArch32.TakeMonitorTrapException(); elsif HaveEL(EL3) && !ELUsingAArch32(EL3) && MDCR_EL3.TDA == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.AArch32SystemAccessTrap(EL3, 0x05); else R[t] = DBGDCCINT; elsif PSTATE.EL == EL3 then if PSTATE.M != M32_Monitor && SDCR.TDCC == '1' then AArch32.TakeMonitorTrapException(); else R[t] = DBGDCCINT;

#### MCR{<c>}{<q>} <coproc>, {#}<opc1>, <Rt>, <CRn>, <CRm>{, {#}<opc2>}

coproc | opc1 | CRn | CRm | opc2
--- | --- | --- | --- | ---
0b1110 | 0b000 | 0b0000 | 0b0010 | 0b000

if PSTATE.EL == EL0 then UNDEFINED; elsif Halted() && ConstrainUnpredictableBool(Unpredictable_IGNORETRAPINDEBUG) then DBGDCCINT = R[t]; elsif PSTATE.EL == EL1 then if HaveEL(EL3) && EL3SDDUndefPriority() && !ELUsingAArch32(EL3) && IsFeatureImplemented(FEAT_FGT) && MDCR_EL3.TDCC == '1' then UNDEFINED; elsif HaveEL(EL3) && EL3SDDUndefPriority() && ELUsingAArch32(EL3) && SDCR.TDCC == '1' then UNDEFINED; elsif HaveEL(EL3) && EL3SDDUndefPriority() && !ELUsingAArch32(EL3) && MDCR_EL3.TDA == '1' then UNDEFINED; elsif EL2Enabled() && !ELUsingAArch32(EL2) && IsFeatureImplemented(FEAT_FGT) && MDCR_EL2.TDCC == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x05); elsif EL2Enabled() && ELUsingAArch32(EL2) && HDCR.TDCC == '1' then AArch32.TakeHypTrapException(0x05); elsif EL2Enabled() && !ELUsingAArch32(EL2) && MDCR_EL2.<TDE,TDA> != '00' then AArch64.AArch32SystemAccessTrap(EL2, 0x05); elsif EL2Enabled() && ELUsingAArch32(EL2) && HDCR.<TDE,TDA> != '00' then AArch32.TakeHypTrapException(0x05); elsif HaveEL(EL3) && !ELUsingAArch32(EL3) && IsFeatureImplemented(FEAT_FGT) && MDCR_EL3.TDCC == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.AArch32SystemAccessTrap(EL3, 0x05); elsif HaveEL(EL3) && ELUsingAArch32(EL3) && SDCR.TDCC == '1' then if EL3SDDUndef() then UNDEFINED; else AArch32.TakeMonitorTrapException(); elsif HaveEL(EL3) && !ELUsingAArch32(EL3) && MDCR_EL3.TDA == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.AArch32SystemAccessTrap(EL3, 0x05); else DBGDCCINT = R[t]; elsif PSTATE.EL == EL2 then if HaveEL(EL3) && EL3SDDUndefPriority() && !ELUsingAArch32(EL3) && IsFeatureImplemented(FEAT_FGT) && MDCR_EL3.TDCC == '1' then UNDEFINED; elsif HaveEL(EL3) && EL3SDDUndefPriority() && ELUsingAArch32(EL3) && SDCR.TDCC == '1' then UNDEFINED; elsif HaveEL(EL3) && EL3SDDUndefPriority() && !ELUsingAArch32(EL3) && MDCR_EL3.TDA == '1' then UNDEFINED; elsif HaveEL(EL3) && !ELUsingAArch32(EL3) && IsFeatureImplemented(FEAT_FGT) && MDCR_EL3.TDCC == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.AArch32SystemAccessTrap(EL3, 0x05); elsif HaveEL(EL3) && ELUsingAArch32(EL3) && SDCR.TDCC == '1' then if EL3SDDUndef() then UNDEFINED; else AArch32.TakeMonitorTrapException(); elsif HaveEL(EL3) && !ELUsingAArch32(EL3) && MDCR_EL3.TDA == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.AArch32SystemAccessTrap(EL3, 0x05); else DBGDCCINT = R[t]; elsif PSTATE.EL == EL3 then if PSTATE.M != M32_Monitor && SDCR.TDCC == '1' then AArch32.TakeMonitorTrapException(); else DBGDCCINT = R[t];

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.