Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## MLS (by element)

Multiply-Subtract from accumulator (vector, by element). This instruction multiplies the vector elements in the first source SIMD&FP register by the specified value in the second source SIMD&FP register, and subtracts the results from the vector elements of the destination SIMD&FP register. All the values in this instruction are unsigned integer values.

Depending on the settings in the CPACR_EL1, CPTR_EL2, and CPTR_EL3 registers, and the current Security state and Exception level, an attempt to execute the instruction might be trapped.

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | Q | 1 | 0 | 1 | 1 | 1 | 1 | size | L | M | Rm | 0 | 1 | 0 | 0 | H | 0 | Rn | Rd
|  |  |  |  |  |  |  |  | o2 |  |  |  |  |

####

MLS <Vd>.<T>, <Vn>.<T>, <Vm>.<Ts>[<index>]

constant integer idxdsize = 64 << UInt(H); integer index; bit Rmhi; case size of when '01' index = UInt(H:L:M); Rmhi = '0'; when '10' index = UInt(H:L); Rmhi = M; otherwise UNDEFINED; integer d = UInt(Rd); integer n = UInt(Rn); integer m = UInt(Rmhi:Rm); constant integer esize = 8 << UInt(size); constant integer datasize = 64 << UInt(Q); integer elements = datasize DIV esize; boolean sub_op = (o2 == '1');

### Assembler Symbols

<Vd> | Is the name of the SIMD&FP destination register, encoded in the "Rd" field.

<T> | Is an arrangement specifier, encoded in size:Q:
size | Q | <T>
--- | --- | ---
00 | x | RESERVED
01 | 0 | 4H
01 | 1 | 8H
10 | 0 | 2S
10 | 1 | 4S
11 | x | RESERVED

<Vn> | Is the name of the first SIMD&FP source register, encoded in the "Rn" field.

<Vm> | Is the name of the second SIMD&FP source register, encoded in size:M:Rm:
size | <Vm>
--- | ---
00 | RESERVED
01 | 0:Rm
10 | M:Rm
11 | RESERVED
Restricted to V0-V15 when element size <Ts> is H.

<Ts> | Is an element size specifier, encoded in size:
size | <Ts>
--- | ---
00 | RESERVED
01 | H
10 | S
11 | RESERVED

<index> | Is the element index, encoded in size:L:H:M:
size | <index>
--- | ---
00 | RESERVED
01 | H:L:M
10 | H:L
11 | RESERVED

### Operation

CheckFPAdvSIMDEnabled64(); bits(datasize) operand1 = V[n, datasize]; bits(idxdsize) operand2 = V[m, idxdsize]; bits(datasize) operand3 = V[d, datasize]; bits(datasize) result; integer element1; integer element2; bits(esize) product; element2 = UInt(Elem[operand2, index, esize]); for e = 0 to elements-1 element1 = UInt(Elem[operand1, e, esize]); product = (element1*element2)<esize-1:0>; if sub_op then Elem[result, e, esize] = Elem[operand3, e, esize] - product; else Elem[result, e, esize] = Elem[operand3, e, esize] + product; V[d, datasize] = result;

### Operational information

If PSTATE.DIT is 1:

- The execution time of this instruction is independent of:
  - The values of the data supplied in any of its registers.
  - The values of the NZCV flags.
- The response of this instruction to asynchronous exceptions does not vary based on:
  - The values of the data supplied in any of its registers.
  - The values of the NZCV flags.

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: isa v33.74, AdvSIMD v29.23, pseudocode v2023-09_rel, sve v2023-09_rc3 ; Build timestamp: 2023-09-27T17:06

Copyright © 2010-2023 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.