Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## LD1RQB (scalar plus immediate)

Contiguous load and replicate sixteen bytes (immediate index)

Load sixteen contiguous bytes to elements of a short, 128-bit (quadword) vector from the memory address generated by a 64-bit scalar base address and immediate index that is a multiple of 16 in the range -128 to +112 added to the base address.

Inactive elements will not cause a read from Device memory or signal a fault, and are set to zero. The resulting short vector is then replicated to fill the long destination vector. Only the first sixteen predicate elements are used and higher numbered predicate elements are ignored.

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
1 | 0 | 1 | 0 | 0 | 1 | 0 | 0 | 0 | 0 | 0 | 0 | imm4 | 0 | 0 | 1 | Pg | Rn | Zt
| msz<1> | msz<0> | ssz |  |  |  |  |  |

####

LD1RQB { <Zt>.B }, <Pg>/Z, [<Xn|SP>{, #<imm>}]

if !HaveSVE() && !HaveSME() then UNDEFINED; integer t = UInt(Zt); integer n = UInt(Rn); integer g = UInt(Pg); constant integer esize = 8; integer offset = SInt(imm4);

### Assembler Symbols

<Zt> | Is the name of the scalable vector register to be transferred, encoded in the "Zt" field.

<Pg> | Is the name of the governing scalable predicate register P0-P7, encoded in the "Pg" field.

<Xn|SP> | Is the 64-bit name of the general-purpose base register or stack pointer, encoded in the "Rn" field.

<imm> | Is the optional signed immediate byte offset, a multiple of 16 in the range -128 to 112, defaulting to 0, encoded in the "imm4" field.

### Operation

CheckSVEEnabled(); constant integer VL = CurrentVL; constant integer PL = VL DIV 8; constant integer elements = 128 DIV esize; bits(64) base; bits(PL) mask = P[g, PL]; // low 16 bits only bits(128) result; constant integer mbytes = esize DIV 8; boolean contiguous = TRUE; boolean nontemporal = FALSE; boolean tagchecked = n != 31; AccessDescriptor accdesc = CreateAccDescSVE(MemOp_LOAD, nontemporal, contiguous, tagchecked); if !AnyActiveElement(mask, esize) then if n == 31 && ConstrainUnpredictableBool(Unpredictable_CHECKSPNONEACTIVE) then CheckSPAlignment(); else if n == 31 then CheckSPAlignment(); base = if n == 31 then SP[] else X[n, 64]; for e = 0 to elements-1 if ElemP[mask, e, esize] == '1' then bits(64) addr = base + (offset * 16) + (e * mbytes); Elem[result, e, esize] = Mem[addr, mbytes, accdesc]; else Elem[result, e, esize] = Zeros(esize); Z[t, VL] = Replicate(result, VL DIV 128);

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: isa v33.53, AdvSIMD v29.11, pseudocode v2022-09_rel, sve v2022-09_rel ; Build timestamp: 2022-09-30T16:37

Copyright © 2010-2022 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.