AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# TRCCCCTLR, Trace Cycle Count Control Register

The TRCCCCTLR characteristics are:

## Purpose

Set the threshold value for cycle counting.

## Configuration

AArch64 System register TRCCCCTLR bits [31:0] are architecturally mapped to External register TRCCCCTLR[31:0].

This register is present only when FEAT_ETE is implemented, System register access to the trace unit registers is implemented and TRCIDR0.TRCCCI == 1. Otherwise, direct accesses to TRCCCCTLR are UNDEFINED.

## Attributes

TRCCCCTLR is a 64-bit register.

## Field descriptions

63 | 62 | 61 | 60 | 59 | 58 | 57 | 56 | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48 | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40 | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
RES0
RES0 | THRESHOLD

#### Bits [63:12]

Reserved, RES0.

#### THRESHOLD, bits [11:0]

Sets the threshold value for instruction trace cycle counting.

The minimum threshold value that can be programmed into THRESHOLD is given in TRCIDR3.CCITMIN. If the THRESHOLD value is smaller than the value in TRCIDR3.CCITMIN then the behavior is CONSTRAINED UNPREDICTABLE. That is, cycle counts might or might not be included in the trace and the cycle count threshold is not known.

Writing a value of zero when TRCCONFIGR.CCI enables instruction trace cycle counting results in CONSTRAINED UNPREDICTABLE behavior. That is, cycle counts might or might not be included in the trace and the cycle count threshold is not known.

The reset behavior of this field is:

- On a Trace unit reset, this field resets to an architecturally UNKNOWN value.

## Accessing TRCCCCTLR

Must be programmed if TRCCONFIGR.CCI == 1.

Writes are CONSTRAINED UNPREDICTABLE if the trace unit is not in the Idle state.

Accesses to this register use the following encodings in the System register encoding space:

#### MRS <Xt>, TRCCCCTLR

op0 | op1 | CRn | CRm | op2
--- | --- | --- | --- | ---
0b10 | 0b001 | 0b0000 | 0b1110 | 0b000

if PSTATE.EL == EL0 then UNDEFINED; elsif PSTATE.EL == EL1 then if HaveEL(EL3) && EL3SDDUndefPriority() && CPTR_EL3.TTA == '1' then UNDEFINED; elsif CPACR_EL1.TTA == '1' then AArch64.SystemAccessTrap(EL1, 0x18); elsif EL2Enabled() && CPTR_EL2.TTA == '1' then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && IsFeatureImplemented(FEAT_FGT) && (!HaveEL(EL3) || SCR_EL3.FGTEn == '1') && HDFGRTR_EL2.TRC == '1' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && CPTR_EL3.TTA == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif IsFeatureImplemented(FEAT_TRBE_EXT) && OSLSR_EL1.OSLK == '0' && HaltingAllowed() && EDSCR2.TTA == '1' then Halt(DebugHalt_SoftwareAccess); else X[t, 64] = TRCCCCTLR; elsif PSTATE.EL == EL2 then if HaveEL(EL3) && EL3SDDUndefPriority() && CPTR_EL3.TTA == '1' then UNDEFINED; elsif CPTR_EL2.TTA == '1' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && CPTR_EL3.TTA == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif !ELUsingAArch32(EL1) && IsFeatureImplemented(FEAT_TRBE_EXT) && OSLSR_EL1.OSLK == '0' && HaltingAllowed() && EDSCR2.TTA == '1' then Halt(DebugHalt_SoftwareAccess); else X[t, 64] = TRCCCCTLR; elsif PSTATE.EL == EL3 then if CPTR_EL3.TTA == '1' then AArch64.SystemAccessTrap(EL3, 0x18); elsif !ELUsingAArch32(EL1) && IsFeatureImplemented(FEAT_TRBE_EXT) && OSLSR_EL1.OSLK == '0' && HaltingAllowed() && EDSCR2.TTA == '1' then Halt(DebugHalt_SoftwareAccess); else X[t, 64] = TRCCCCTLR;

#### MSR TRCCCCTLR, <Xt>

op0 | op1 | CRn | CRm | op2
--- | --- | --- | --- | ---
0b10 | 0b001 | 0b0000 | 0b1110 | 0b000

if PSTATE.EL == EL0 then UNDEFINED; elsif PSTATE.EL == EL1 then if HaveEL(EL3) && EL3SDDUndefPriority() && CPTR_EL3.TTA == '1' then UNDEFINED; elsif CPACR_EL1.TTA == '1' then AArch64.SystemAccessTrap(EL1, 0x18); elsif EL2Enabled() && CPTR_EL2.TTA == '1' then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && IsFeatureImplemented(FEAT_FGT) && (!HaveEL(EL3) || SCR_EL3.FGTEn == '1') && HDFGWTR_EL2.TRC == '1' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && CPTR_EL3.TTA == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif IsFeatureImplemented(FEAT_TRBE_EXT) && OSLSR_EL1.OSLK == '0' && HaltingAllowed() && EDSCR2.TTA == '1' then Halt(DebugHalt_SoftwareAccess); else TRCCCCTLR = X[t, 64]; elsif PSTATE.EL == EL2 then if HaveEL(EL3) && EL3SDDUndefPriority() && CPTR_EL3.TTA == '1' then UNDEFINED; elsif CPTR_EL2.TTA == '1' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && CPTR_EL3.TTA == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif !ELUsingAArch32(EL1) && IsFeatureImplemented(FEAT_TRBE_EXT) && OSLSR_EL1.OSLK == '0' && HaltingAllowed() && EDSCR2.TTA == '1' then Halt(DebugHalt_SoftwareAccess); else TRCCCCTLR = X[t, 64]; elsif PSTATE.EL == EL3 then if CPTR_EL3.TTA == '1' then AArch64.SystemAccessTrap(EL3, 0x18); elsif !ELUsingAArch32(EL1) && IsFeatureImplemented(FEAT_TRBE_EXT) && OSLSR_EL1.OSLK == '0' && HaltingAllowed() && EDSCR2.TTA == '1' then Halt(DebugHalt_SoftwareAccess); else TRCCCCTLR = X[t, 64];

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.