Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## ZIP1

Zip vectors (primary). This instruction reads adjacent vector elements from the lower half of two source SIMD&FP registers as pairs, interleaves the pairs and places them into a vector, and writes the vector to the destination SIMD&FP register. The first pair from the first source register is placed into the two lowest vector elements, with subsequent pairs taken alternately from each source register.

#### Note

This instruction can be used with ZIP2 to interleave two vectors.

The following figure shows an example of the operation of ZIP1 and ZIP2 with the arrangement specifier 8B.

Depending on the settings in the CPACR_EL1, CPTR_EL2, and CPTR_EL3 registers, and the current Security state and Exception level, an attempt to execute the instruction might be trapped.

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | Q | 0 | 0 | 1 | 1 | 1 | 0 | size | 0 | Rm | 0 | 0 | 1 | 1 | 1 | 0 | Rn | Rd
|  |  |  |  |  |  | op |  |  |

####

ZIP1 <Vd>.<T>, <Vn>.<T>, <Vm>.<T>

integer d = UInt(Rd); integer n = UInt(Rn); integer m = UInt(Rm); if size:Q == '110' then UNDEFINED; constant integer esize = 8 << UInt(size); constant integer datasize = 64 << UInt(Q); integer elements = datasize DIV esize; integer part = UInt(op); integer pairs = elements DIV 2;

### Assembler Symbols

<Vd> | Is the name of the SIMD&FP destination register, encoded in the "Rd" field.

<T> | Is an arrangement specifier, encoded in size:Q:
size | Q | <T>
--- | --- | ---
00 | 0 | 8B
00 | 1 | 16B
01 | 0 | 4H
01 | 1 | 8H
10 | 0 | 2S
10 | 1 | 4S
11 | 0 | RESERVED
11 | 1 | 2D

<Vn> | Is the name of the first SIMD&FP source register, encoded in the "Rn" field.

<Vm> | Is the name of the second SIMD&FP source register, encoded in the "Rm" field.

### Operation

CheckFPAdvSIMDEnabled64(); bits(datasize) operand1 = V[n, datasize]; bits(datasize) operand2 = V[m, datasize]; bits(datasize) result; integer base = part * pairs; for p = 0 to pairs-1 Elem[result, 2*p+0, esize] = Elem[operand1, base+p, esize]; Elem[result, 2*p+1, esize] = Elem[operand2, base+p, esize]; V[d, datasize] = result;

### Operational information

If PSTATE.DIT is 1:

- The execution time of this instruction is independent of:
  - The values of the data supplied in any of its registers.
  - The values of the NZCV flags.
- The response of this instruction to asynchronous exceptions does not vary based on:
  - The values of the data supplied in any of its registers.
  - The values of the NZCV flags.

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: aarchmrs v2024-03_relA, pseudocode v2024-03_rel, sve v2024-03_rel ; Build timestamp: 2024-03-26T09:45

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.