AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# SPMSELR_EL0, System Performance Monitors Select Register

The SPMSELR_EL0 characteristics are:

## Purpose

Selects the System PMU and event counter registers to access.

## Configuration

This register is present only when FEAT_SPMU is implemented. Otherwise, direct accesses to SPMSELR_EL0 are UNDEFINED.

## Attributes

SPMSELR_EL0 is a 64-bit register.

## Field descriptions

63 | 62 | 61 | 60 | 59 | 58 | 57 | 56 | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48 | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40 | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
RES0
RES0 | SYSPMUSEL | RES0 | BANK

#### Bits [63:10]

Reserved, RES0.

#### SYSPMUSEL, bits [9:4]

System PMU Select. Selects a System PMU <s> to access.

Values 0x20 to 0x3F are reserved.

The reset behavior of this field is:

- On a Warm reset, this field resets to an architecturally UNKNOWN value.

#### Bits [3:2]

Reserved, RES0.

#### BANK, bits [1:0]

System PMU bank access control. Selects a bank of 16 System PMU event counters and related controls to access.

BANK | Meaning
--- | ---
0b00 | Select event counters 0 to 15.
0b01 | Select event counters 16 to 31.
0b10 | Select event counters 32 to 47.
0b11 | Select event counters 48 to 63.

The reset behavior of this field is:

- On a Warm reset, this field resets to an architecturally UNKNOWN value.

## Accessing SPMSELR_EL0

Accesses to this register use the following encodings in the System register encoding space:

#### MRS <Xt>, SPMSELR_EL0

op0 | op1 | CRn | CRm | op2
--- | --- | --- | --- | ---
0b10 | 0b011 | 0b1001 | 0b1100 | 0b101

if PSTATE.EL == EL0 then if HaveEL(EL3) && EL3SDDUndefPriority() && MDCR_EL3.EnPM2 == '0' then UNDEFINED; elsif MDSCR_EL1.EnSPM == '0' then if EL2Enabled() && HCR_EL2.TGE == '1' then AArch64.SystemAccessTrap(EL2, 0x18); else AArch64.SystemAccessTrap(EL1, 0x18); elsif EL2Enabled() && !ELIsInHost(EL0) && IsFeatureImplemented(FEAT_FGT2) && HaveEL(EL3) && SCR_EL3.FGTEn2 == '0' then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && !ELIsInHost(EL0) && IsFeatureImplemented(FEAT_FGT2) && HDFGRTR2_EL2.nSPMSELR_EL0 == '0' then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && MDCR_EL2.EnSPM == '0' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && MDCR_EL3.EnPM2 == '0' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); else X[t, 64] = SPMSELR_EL0; elsif PSTATE.EL == EL1 then if HaveEL(EL3) && EL3SDDUndefPriority() && MDCR_EL3.EnPM2 == '0' then UNDEFINED; elsif EL2Enabled() && IsFeatureImplemented(FEAT_FGT2) && ((HaveEL(EL3) && SCR_EL3.FGTEn2 == '0') || HDFGRTR2_EL2.nSPMSELR_EL0 == '0') then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && MDCR_EL2.EnSPM == '0' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && MDCR_EL3.EnPM2 == '0' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); else X[t, 64] = SPMSELR_EL0; elsif PSTATE.EL == EL2 then if HaveEL(EL3) && EL3SDDUndefPriority() && MDCR_EL3.EnPM2 == '0' then UNDEFINED; elsif HaveEL(EL3) && MDCR_EL3.EnPM2 == '0' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); else X[t, 64] = SPMSELR_EL0; elsif PSTATE.EL == EL3 then X[t, 64] = SPMSELR_EL0;

#### MSR SPMSELR_EL0, <Xt>

op0 | op1 | CRn | CRm | op2
--- | --- | --- | --- | ---
0b10 | 0b011 | 0b1001 | 0b1100 | 0b101

if PSTATE.EL == EL0 then if HaveEL(EL3) && EL3SDDUndefPriority() && MDCR_EL3.EnPM2 == '0' then UNDEFINED; elsif MDSCR_EL1.EnSPM == '0' then if EL2Enabled() && HCR_EL2.TGE == '1' then AArch64.SystemAccessTrap(EL2, 0x18); else AArch64.SystemAccessTrap(EL1, 0x18); elsif EL2Enabled() && !ELIsInHost(EL0) && IsFeatureImplemented(FEAT_FGT2) && HaveEL(EL3) && SCR_EL3.FGTEn2 == '0' then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && !ELIsInHost(EL0) && IsFeatureImplemented(FEAT_FGT2) && HDFGWTR2_EL2.nSPMSELR_EL0 == '0' then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && MDCR_EL2.EnSPM == '0' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && MDCR_EL3.EnPM2 == '0' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); else SPMSELR_EL0 = X[t, 64]; elsif PSTATE.EL == EL1 then if HaveEL(EL3) && EL3SDDUndefPriority() && MDCR_EL3.EnPM2 == '0' then UNDEFINED; elsif EL2Enabled() && IsFeatureImplemented(FEAT_FGT2) && ((HaveEL(EL3) && SCR_EL3.FGTEn2 == '0') || HDFGWTR2_EL2.nSPMSELR_EL0 == '0') then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && MDCR_EL2.EnSPM == '0' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && MDCR_EL3.EnPM2 == '0' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); else SPMSELR_EL0 = X[t, 64]; elsif PSTATE.EL == EL2 then if HaveEL(EL3) && EL3SDDUndefPriority() && MDCR_EL3.EnPM2 == '0' then UNDEFINED; elsif HaveEL(EL3) && MDCR_EL3.EnPM2 == '0' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); else SPMSELR_EL0 = X[t, 64]; elsif PSTATE.EL == EL3 then SPMSELR_EL0 = X[t, 64];

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.