AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# GICR_IGRPMODR0, Interrupt Group Modifier Register 0

The GICR_IGRPMODR0 characteristics are:

## Purpose

When GICD_CTLR.DS==0, this register together with the GICR_IGROUPR0 register, controls whether the corresponding interrupt is in:

- Secure Group 0.
- Non-secure Group 1.
- When System register access is enabled, Secure Group 1.

## Configuration

When GICD_CTLR.DS==0, this register is Secure.

A copy of this register is provided for each Redistributor.

## Attributes

GICR_IGRPMODR0 is a 32-bit register.

## Field descriptions

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
Group_modifier_bit31 | Group_modifier_bit30 | Group_modifier_bit29 | Group_modifier_bit28 | Group_modifier_bit27 | Group_modifier_bit26 | Group_modifier_bit25 | Group_modifier_bit24 | Group_modifier_bit23 | Group_modifier_bit22 | Group_modifier_bit21 | Group_modifier_bit20 | Group_modifier_bit19 | Group_modifier_bit18 | Group_modifier_bit17 | Group_modifier_bit16 | Group_modifier_bit15 | Group_modifier_bit14 | Group_modifier_bit13 | Group_modifier_bit12 | Group_modifier_bit11 | Group_modifier_bit10 | Group_modifier_bit9 | Group_modifier_bit8 | Group_modifier_bit7 | Group_modifier_bit6 | Group_modifier_bit5 | Group_modifier_bit4 | Group_modifier_bit3 | Group_modifier_bit2 | Group_modifier_bit1 | Group_modifier_bit0

#### Group_modifier_bit<x>, bit [x], for x = 31 to 0

Group modifier bit. In implementations where affinity routing is enabled for the Security state of an interrupt, the bit that corresponds to the interrupt is concatenated with the equivalent bit in GICR_IGROUPR0 to form a 2-bit field that defines an interrupt group:

Group modifier bit | Group status bit | Definition | Short name
--- | --- | --- | ---
0b0 | 0b0 | Secure Group 0 | G0S
0b0 | 0b1 | Non-secure Group 1 | G1NS
0b1 | 0b0 | Secure Group 1 | G1S
0b1 | 0b1 | Reserved, treated as Non-secure Group 1 | -

The reset behavior of this field is:

- On a GIC reset, this field resets to an architecturally UNKNOWN value.

## Accessing GICR_IGRPMODR0

When affinity routing is not enabled for the Security state of an interrupt in GICR_IGRPMODR0, the corresponding bit is RES0 and equivalent functionality is provided by GICD_IGRPMODR<n> with n=0.

This register only applies to SGIs (bits [15:0]) and PPIs (bits [31:16]). For SPIs, this functionality is provided by GICD_IGRPMODR<n>.

When GICD_CTLR.ARE_S == 0 or GICD_CTLR.DS == 1, GICR_IGRPMODR0 is RES0. An implementation can make this register RAZ/WI in this case.

When GICD_CTLR.DS==0, the register is RAZ/WI to Non-secure accesses.

Bits corresponding to unimplemented interrupts are RAZ/WI.

Note

Implementations must ensure that an interrupt that is pending at the time of the write uses either the old value or the new value and must ensure that the interrupt is neither lost nor handled more than one time. The effect of the change must be visible in finite time.

#### GICR_IGRPMODR0 can be accessed through the memory-mapped interfaces:

Component | Frame | Offset | Instance
--- | --- | --- | ---
GIC Redistributor | SGI_base | 0x0D00 | GICR_IGRPMODR0

Accesses on this interface are RW.

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.