AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# ERRIDR_EL1, Error Record ID Register

The ERRIDR_EL1 characteristics are:

## Purpose

Defines the highest numbered index of the error records that can be accessed through the Error Record System registers.

## Configuration

AArch64 System register ERRIDR_EL1 bits [31:0] are architecturally mapped to AArch32 System register ERRIDR[31:0].

This register is present only when FEAT_RAS is implemented. Otherwise, direct accesses to ERRIDR_EL1 are UNDEFINED.

## Attributes

ERRIDR_EL1 is a 64-bit register.

## Field descriptions

63 | 62 | 61 | 60 | 59 | 58 | 57 | 56 | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48 | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40 | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
RES0
RES0 | NUM

#### Bits [63:16]

Reserved, RES0.

#### NUM, bits [15:0]

Highest numbered index of the records that can be accessed through the Error Record System registers plus one. Zero indicates no records can be accessed through the Error Record System registers.

Each implemented record is owned by a node. A node might own multiple records.

This field has an IMPLEMENTATION DEFINED value.

Access to this field is RO.

## Accessing ERRIDR_EL1

Accesses to this register use the following encodings in the System register encoding space:

#### MRS <Xt>, ERRIDR_EL1

op0 | op1 | CRn | CRm | op2
--- | --- | --- | --- | ---
0b11 | 0b000 | 0b0101 | 0b0011 | 0b000

if PSTATE.EL == EL0 then UNDEFINED; elsif PSTATE.EL == EL1 then if HaveEL(EL3) && EL3SDDUndefPriority() && SCR_EL3.TERR == '1' then UNDEFINED; elsif EL2Enabled() && HCR_EL2.TERR == '1' then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && IsFeatureImplemented(FEAT_FGT) && (!HaveEL(EL3) || SCR_EL3.FGTEn == '1') && HFGRTR_EL2.ERRIDR_EL1 == '1' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && SCR_EL3.TERR == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); else X[t, 64] = ERRIDR_EL1; elsif PSTATE.EL == EL2 then if HaveEL(EL3) && EL3SDDUndefPriority() && SCR_EL3.TERR == '1' then UNDEFINED; elsif HaveEL(EL3) && SCR_EL3.TERR == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); else X[t, 64] = ERRIDR_EL1; elsif PSTATE.EL == EL3 then X[t, 64] = ERRIDR_EL1;

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.