Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## UXTB, UXTH, UXTW

Unsigned byte / halfword / word extend (predicated)

Zero-extend the least-significant sub-element of each active element of the source vector, and place the results in the corresponding elements of the destination vector. Inactive elements in the destination vector register remain unmodified.

It has encodings from 3 classes: Byte , Halfword and Word

### Byte

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | 0 | 0 | 0 | 0 | 1 | 0 | 0 | size | 0 | 1 | 0 | 0 | 0 | 1 | 1 | 0 | 1 | Pg | Zn | Zd
|  |  |  | U |  |  |  |

####

UXTB <Zd>.<T>, <Pg>/M, <Zn>.<T>

if !HaveSVE() && !HaveSME() then UNDEFINED; if size == '00' then UNDEFINED; constant integer esize = 8 << UInt(size); constant integer s_esize = 8; integer g = UInt(Pg); integer n = UInt(Zn); integer d = UInt(Zd); boolean unsigned = TRUE;

### Halfword

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | 0 | 0 | 0 | 0 | 1 | 0 | 0 | size | 0 | 1 | 0 | 0 | 1 | 1 | 1 | 0 | 1 | Pg | Zn | Zd
|  |  |  | U |  |  |  |

####

UXTH <Zd>.<T>, <Pg>/M, <Zn>.<T>

if !HaveSVE() && !HaveSME() then UNDEFINED; if size IN {'0x'} then UNDEFINED; constant integer esize = 8 << UInt(size); constant integer s_esize = 16; integer g = UInt(Pg); integer n = UInt(Zn); integer d = UInt(Zd); boolean unsigned = TRUE;

### Word

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | 0 | 0 | 0 | 0 | 1 | 0 | 0 | size | 0 | 1 | 0 | 1 | 0 | 1 | 1 | 0 | 1 | Pg | Zn | Zd
|  |  |  | U |  |  |  |

####

UXTW <Zd>.D, <Pg>/M, <Zn>.D

if !HaveSVE() && !HaveSME() then UNDEFINED; if size != '11' then UNDEFINED; constant integer esize = 8 << UInt(size); constant integer s_esize = 32; integer g = UInt(Pg); integer n = UInt(Zn); integer d = UInt(Zd); boolean unsigned = TRUE;

### Assembler Symbols

<Zd> | Is the name of the destination scalable vector register, encoded in the "Zd" field.

<T> | For the byte variant: is the size specifier, encoded in size:
size | <T>
--- | ---
00 | RESERVED
01 | H
10 | S
11 | D
| For the halfword variant: is the size specifier, encoded in size<0>:
size<0> | <T>
--- | ---
0 | S
1 | D

<Pg> | Is the name of the governing scalable predicate register P0-P7, encoded in the "Pg" field.

<Zn> | Is the name of the source scalable vector register, encoded in the "Zn" field.

### Operation

CheckSVEEnabled(); constant integer VL = CurrentVL; constant integer PL = VL DIV 8; constant integer elements = VL DIV esize; bits(PL) mask = P[g, PL]; bits(VL) operand = if AnyActiveElement(mask, esize) then Z[n, VL] else Zeros(VL); bits(VL) result = Z[d, VL]; for e = 0 to elements-1 if ElemP[mask, e, esize] == '1' then bits(esize) element = Elem[operand, e, esize]; Elem[result, e, esize] = Extend(element<s_esize-1:0>, esize, unsigned); Z[d, VL] = result;

### Operational information

If FEAT_SVE2 is implemented or FEAT_SME is implemented, then when PSTATE.DIT is 1:

- The execution time of this instruction is independent of:
  - The values of the data supplied in any of its operand registers when its governing predicate register contains the same value for each execution.
  - The values of the NZCV flags.
- The response of this instruction to asynchronous exceptions does not vary based on:
  - The values of the data supplied in any of its operand registers when its governing predicate register contains the same value for each execution.
  - The values of the NZCV flags.

This instruction might be immediately preceded in program order by a MOVPRFX instruction. The MOVPRFX instruction must conform to all of the following requirements, otherwise the behavior of the MOVPRFX and this instruction is unpredictable:

- The MOVPRFX instruction must be unpredicated, or be predicated using the same governing predicate register and source element size as this instruction.
- The MOVPRFX instruction must specify the same destination register as this instruction.
- The destination register must not refer to architectural register state referenced by any other source operand register of this instruction.

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: isa v33.53, AdvSIMD v29.11, pseudocode v2022-09_rel, sve v2022-09_rel ; Build timestamp: 2022-09-30T16:37

Copyright © 2010-2022 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.