Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## FDOT (2-way, vector)

8-bit floating-point dot product to half-precision (vector). This instruction computes the fused sum-of-products of a group of two 8-bit floating-point values held in each 16-bit element of the first and second source vectors. The half-precision sum-of-products are scaled by 2-UInt(FPMR.LSCALE[3:0]), before being destructively added without intermediate rounding to the corresponding half-precision elements of the destination vector.

The 8-bit floating-point encoding format for the elements of the first source vector is selected by FPMR.F8S1. The 8-bit floating-point encoding format for the elements of the second source vector is selected by FPMR.F8S2.

### Advanced SIMD
(FEAT_FP8DOT2)

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | Q | 0 | 0 | 1 | 1 | 1 | 0 | 0 | 1 | 0 | Rm | 1 | 1 | 1 | 1 | 1 | 1 | Rn | Rd

####

FDOT <Vd>.<Ta>, <Vn>.<Tb>, <Vm>.<Tb>

if !IsFeatureImplemented(FEAT_FP8DOT2) then UNDEFINED; integer n = UInt(Rn); integer m = UInt(Rm); integer d = UInt(Rd); constant integer datasize = if Q == '1' then 128 else 64; constant integer esize = 16; constant integer elements = datasize DIV esize;

### Assembler Symbols

<Vd> | Is the name of the SIMD&FP destination register, encoded in the "Rd" field.

<Ta> | Is an arrangement specifier, encoded in Q:
Q | <Ta>
--- | ---
0 | 4H
1 | 8H

<Vn> | Is the name of the first SIMD&FP source register, encoded in the "Rn" field.

<Tb> | Is an arrangement specifier, encoded in Q:
Q | <Tb>
--- | ---
0 | 8B
1 | 16B

<Vm> | Is the name of the second SIMD&FP source register, encoded in the "Rm" field.

### Operation

CheckFPMREnabled(); CheckFPAdvSIMDEnabled64(); bits(datasize) operand1 = V[n, datasize]; bits(datasize) operand2 = V[m, datasize]; bits(datasize) operand3 = V[d, datasize]; bits(datasize) result; for e = 0 to elements-1 bits(esize) op1 = Elem[operand1, e, esize]; bits(esize) op2 = Elem[operand2, e, esize]; bits(esize) sum = Elem[operand3, e, esize]; sum = FP8DotAddFP(sum, op1, op2, FPCR, FPMR); Elem[result, e, esize] = sum; V[d, datasize] = result;

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: isa v33.74, AdvSIMD v29.23, pseudocode v2023-09_rel, sve v2023-09_rc3 ; Build timestamp: 2023-09-27T17:06

Copyright © 2010-2023 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.