AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# GICR_STATUSR, Error Reporting Status Register

The GICR_STATUSR characteristics are:

## Purpose

Provides software with a mechanism to detect:

- Accesses to reserved locations.
- Writes to read-only locations.
- Reads of write-only locations.

## Configuration

A copy of this register is provided for each Redistributor.

If the GIC implementation supports two Security states this register is Banked to provide Secure and Non-secure copies.

## Attributes

GICR_STATUSR is a 32-bit register.

## Field descriptions

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
RES0 | WROD | RWOD | WRD | RRD

#### Bits [31:4]

Reserved, RES0.

#### WROD, bit [3]

Write to an RO location.

WROD | Meaning
--- | ---
0b0 | Normal operation.
0b1 | A write to an RO location has been detected.

When a violation is detected, software must write 1 to this register to reset it.

#### RWOD, bit [2]

Read of a WO location.

RWOD | Meaning
--- | ---
0b0 | Normal operation.
0b1 | A read of a WO location has been detected.

When a violation is detected, software must write 1 to this register to reset it.

#### WRD, bit [1]

Write to a reserved location.

WRD | Meaning
--- | ---
0b0 | Normal operation.
0b1 | A write to a reserved location has been detected.

When a violation is detected, software must write 1 to this register to reset it.

#### RRD, bit [0]

Read of a reserved location.

RRD | Meaning
--- | ---
0b0 | Normal operation.
0b1 | A read of a reserved location has been detected.

When a violation is detected, software must write 1 to this register to reset it.

## Accessing GICR_STATUSR

This is an optional register. If the register is not implemented, the location is RAZ/WI.

#### GICR_STATUSR can be accessed through the memory-mapped interfaces:

Component | Frame | Offset | Instance
--- | --- | --- | ---
GIC Redistributor | RD_base | 0x0010 | GICR_STATUSR (S)

This interface is accessible as follows:

- When an access is Secure, accesses to this register are RW.
- When FEAT_RME is implemented and an access is Root, accesses to this register are RW.

Component | Frame | Offset | Instance
--- | --- | --- | ---
GIC Redistributor | RD_base | 0x0010 | GICR_STATUSR (NS)

This interface is accessible as follows:

- When an access is Non-secure, accesses to this register are RW.
- When FEAT_RME is implemented and an access is Realm, accesses to this register are RW.

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.