AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# CTIINTACK, CTI Output Trigger Acknowledge register

The CTIINTACK characteristics are:

## Purpose

Can be used to deactivate the output triggers.

## Configuration

CTIINTACK is in the Debug power domain.

## Attributes

CTIINTACK is a 32-bit register.

## Field descriptions

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
ACK31 | ACK30 | ACK29 | ACK28 | ACK27 | ACK26 | ACK25 | ACK24 | ACK23 | ACK22 | ACK21 | ACK20 | ACK19 | ACK18 | ACK17 | ACK16 | ACK15 | ACK14 | ACK13 | ACK12 | ACK11 | ACK10 | ACK9 | ACK8 | ACK7 | ACK6 | ACK5 | ACK4 | ACK3 | ACK2 | ACK1 | ACK0

#### ACK<n>, bit [n], for n = 31 to 0

Acknowledge for output trigger <n>.

Bits [31:N] are RAZ/WI. N is the number of CTI triggers implemented as defined by the CTIDEVID.NUMTRIG field.

If any of the following is true, writes to ACK<n> are ignored:

- n >= CTIDEVID.NUMTRIG, the number of implemented triggers.
- Output trigger n is not active.
- The channel mapping function output, as controlled by CTIOUTEN<n>, is still active.

Otherwise, if any of the following are true, ACK<n> is RES0:

- Output trigger n is not implemented.
- Output trigger n is not connected.
- Output trigger n is self-acknowledging and does not require software acknowledge.

Otherwise, the behavior on writes to ACK<n> is as follows:

ACK<n> | Meaning
--- | ---
0b0 | No effect
0b1 | Deactivate the trigger.

## Accessing CTIINTACK

A debugger must read CTITRIGOUTSTATUS to confirm that the output trigger has been acknowledged before generating any event that must be ordered after the write to CTIINTACK, such as a write to CTIAPPPULSE to activate another trigger.

#### CTIINTACK can be accessed through the external debug interface:

Component | Offset | Instance
--- | --- | ---
CTI | 0x010 | CTIINTACK

This interface is accessible as follows:

- When SoftwareLockStatus(), accesses to this register are WI.
- Otherwise, accesses to this register are WO.

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.