Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## LDNT1H (scalar plus scalar, consecutive registers)

Contiguous load non-temporal of halfwords to multiple consecutive vectors (scalar index)

Contiguous load non-temporal of halfwords to elements of two or four consecutive vector registers from the memory address generated by a 64-bit scalar base and scalar index which is added to the base address. After each element access the index value is incremented, but the index register is not updated.

Inactive elements will not cause a read from Device memory or signal a fault, and are set to zero in the destination vector.

A non-temporal load is a hint to the system that this data is unlikely to be referenced again soon.

It has encodings from 2 classes: Two registers and Four registers

### Two registers
(FEAT_SVE2p1)

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
1 | 0 | 1 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | Rm | 0 | 0 | 1 | PNg | Rn | Zt | 1
|  |  | msz<1> | msz<0> |  |  |  | N

####

LDNT1H { <Zt1>.H-<Zt2>.H }, <PNg>/Z, [<Xn|SP>, <Xm>, LSL #1]

if !IsFeatureImplemented(FEAT_SME2) && !IsFeatureImplemented(FEAT_SVE2p1) then UNDEFINED; constant integer n = UInt(Rn); constant integer m = UInt(Rm); constant integer g = UInt('1':PNg); constant integer nreg = 2; constant integer t = UInt(Zt:'0'); constant integer esize = 16;

### Four registers
(FEAT_SVE2p1)

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
1 | 0 | 1 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | Rm | 1 | 0 | 1 | PNg | Rn | Zt | 0 | 1
|  |  | msz<1> | msz<0> |  |  |  |  | N

####

LDNT1H { <Zt1>.H-<Zt4>.H }, <PNg>/Z, [<Xn|SP>, <Xm>, LSL #1]

if !IsFeatureImplemented(FEAT_SME2) && !IsFeatureImplemented(FEAT_SVE2p1) then UNDEFINED; constant integer n = UInt(Rn); constant integer m = UInt(Rm); constant integer g = UInt('1':PNg); constant integer nreg = 4; constant integer t = UInt(Zt:'00'); constant integer esize = 16;

### Assembler Symbols

<Zt1> | For the two registers variant: is the name of the first scalable vector register to be transferred, encoded as "Zt" times 2.
| For the four registers variant: is the name of the first scalable vector register to be transferred, encoded as "Zt" times 4.

<Zt4> | Is the name of the fourth scalable vector register to be transferred, encoded as "Zt" times 4 plus 3.

<Zt2> | Is the name of the second scalable vector register to be transferred, encoded as "Zt" times 2 plus 1.

<PNg> | Is the name of the governing scalable predicate register PN8-PN15, with predicate-as-counter encoding, encoded in the "PNg" field.

<Xn|SP> | Is the 64-bit name of the general-purpose base register or stack pointer, encoded in the "Rn" field.

<Xm> | Is the 64-bit name of the general-purpose offset register, encoded in the "Rm" field.

### Operation

if IsFeatureImplemented(FEAT_SVE2p1) then CheckSVEEnabled(); else CheckStreamingSVEEnabled(); constant integer VL = CurrentVL; constant integer PL = VL DIV 8; constant integer elements = VL DIV esize; constant integer mbytes = esize DIV 8; bits(64) offset; bits(64) base; bits(64) addr; constant bits(PL) pred = P[g, PL]; constant bits(PL * nreg) mask = CounterToPredicate(pred<15:0>, PL * nreg); array [0..3] of bits(VL) values; constant boolean contiguous = TRUE; constant boolean nontemporal = TRUE; constant integer transfer = t; constant boolean tagchecked = TRUE; constant AccessDescriptor accdesc = CreateAccDescSVE(MemOp_LOAD, nontemporal, contiguous, tagchecked); if !AnyActiveElement(mask, esize) then if n == 31 && ConstrainUnpredictableBool(Unpredictable_CHECKSPNONEACTIVE) then CheckSPAlignment(); else if n == 31 then CheckSPAlignment(); base = if n == 31 then SP[] else X[n, 64]; offset = X[m, 64]; addr = AddressAdd(base, UInt(offset) * mbytes, accdesc); for r = 0 to nreg-1 for e = 0 to elements-1 if ActivePredicateElement(mask, r * elements + e, esize) then Elem[values[r], e, esize] = Mem[addr, mbytes, accdesc]; else Elem[values[r], e, esize] = Zeros(esize); addr = AddressIncrement(addr, mbytes, accdesc); for r = 0 to nreg-1 Z[transfer+r, VL] = values[r];

### Operational information

If PSTATE.DIT is 1, the timing of this instruction is insensitive to the value of the data being loaded or stored when its governing predicate register contains the same value for each execution.

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: aarchmrs v2024-03_relA, pseudocode v2024-03_rel, sve v2024-03_rel ; Build timestamp: 2024-03-26T09:45

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.