AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# TRCCLAIMCLR, Trace Claim Tag Clear Register

The TRCCLAIMCLR characteristics are:

## Purpose

In conjunction with TRCCLAIMSET, provides Claim Tag bits that can be separately set and cleared to indicate whether functionality is in use by a debug agent.

For additional information, see the CoreSight Architecture Specification.

## Configuration

AArch64 System register TRCCLAIMCLR bits [31:0] are architecturally mapped to External register TRCCLAIMCLR[31:0].

This register is present only when FEAT_ETE is implemented and System register access to the trace unit registers is implemented. Otherwise, direct accesses to TRCCLAIMCLR are UNDEFINED.

## Attributes

TRCCLAIMCLR is a 64-bit register.

## Field descriptions

63 | 62 | 61 | 60 | 59 | 58 | 57 | 56 | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48 | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40 | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
RES0
CLR[31] | CLR[30] | CLR[29] | CLR[28] | CLR[27] | CLR[26] | CLR[25] | CLR[24] | CLR[23] | CLR[22] | CLR[21] | CLR[20] | CLR[19] | CLR[18] | CLR[17] | CLR[16] | CLR[15] | CLR[14] | CLR[13] | CLR[12] | CLR[11] | CLR[10] | CLR[9] | CLR[8] | CLR[7] | CLR[6] | CLR[5] | CLR[4] | CLR[3] | CLR[2] | CLR[1] | CLR[0]

#### Bits [63:32]

Reserved, RES0.

#### CLR[<m>], bit [m], for m = 31 to 0

Claim Tag Clear. Indicates the current status of Claim Tag bit <m>, and is used to clear Claim Tag bit <m> to 0.

CLR[<m>] | Meaning
--- | ---
0b0 | On a read: Claim Tag bit <m> is not set. On a write: Ignored.
0b1 | On a read: Claim Tag bit <m> is set. On a write: Clear Claim tag bit <m> to 0.

The number of Claim Tag bits implemented is indicated in TRCCLAIMSET.

This bit reads-as-zero and ignores writes if m > the number of Claim Tag bits.

The reset behavior of this field is:

- On a Trace unit reset, this field resets to 0.

Access to this field is W1C.

## Accessing TRCCLAIMCLR

Accesses to this register use the following encodings in the System register encoding space:

#### MRS <Xt>, TRCCLAIMCLR

op0 | op1 | CRn | CRm | op2
--- | --- | --- | --- | ---
0b10 | 0b001 | 0b0111 | 0b1001 | 0b110

if PSTATE.EL == EL0 then UNDEFINED; elsif PSTATE.EL == EL1 then if HaveEL(EL3) && EL3SDDUndefPriority() && CPTR_EL3.TTA == '1' then UNDEFINED; elsif CPACR_EL1.TTA == '1' then AArch64.SystemAccessTrap(EL1, 0x18); elsif EL2Enabled() && CPTR_EL2.TTA == '1' then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && IsFeatureImplemented(FEAT_FGT) && (!HaveEL(EL3) || SCR_EL3.FGTEn == '1') && HDFGRTR_EL2.TRCCLAIM == '1' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && CPTR_EL3.TTA == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif IsFeatureImplemented(FEAT_TRBE_EXT) && OSLSR_EL1.OSLK == '0' && HaltingAllowed() && EDSCR2.TTA == '1' then Halt(DebugHalt_SoftwareAccess); else X[t, 64] = TRCCLAIMCLR; elsif PSTATE.EL == EL2 then if HaveEL(EL3) && EL3SDDUndefPriority() && CPTR_EL3.TTA == '1' then UNDEFINED; elsif CPTR_EL2.TTA == '1' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && CPTR_EL3.TTA == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif !ELUsingAArch32(EL1) && IsFeatureImplemented(FEAT_TRBE_EXT) && OSLSR_EL1.OSLK == '0' && HaltingAllowed() && EDSCR2.TTA == '1' then Halt(DebugHalt_SoftwareAccess); else X[t, 64] = TRCCLAIMCLR; elsif PSTATE.EL == EL3 then if CPTR_EL3.TTA == '1' then AArch64.SystemAccessTrap(EL3, 0x18); elsif !ELUsingAArch32(EL1) && IsFeatureImplemented(FEAT_TRBE_EXT) && OSLSR_EL1.OSLK == '0' && HaltingAllowed() && EDSCR2.TTA == '1' then Halt(DebugHalt_SoftwareAccess); else X[t, 64] = TRCCLAIMCLR;

#### MSR TRCCLAIMCLR, <Xt>

op0 | op1 | CRn | CRm | op2
--- | --- | --- | --- | ---
0b10 | 0b001 | 0b0111 | 0b1001 | 0b110

if PSTATE.EL == EL0 then UNDEFINED; elsif PSTATE.EL == EL1 then if HaveEL(EL3) && EL3SDDUndefPriority() && CPTR_EL3.TTA == '1' then UNDEFINED; elsif CPACR_EL1.TTA == '1' then AArch64.SystemAccessTrap(EL1, 0x18); elsif EL2Enabled() && CPTR_EL2.TTA == '1' then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && IsFeatureImplemented(FEAT_FGT) && (!HaveEL(EL3) || SCR_EL3.FGTEn == '1') && HDFGWTR_EL2.TRCCLAIM == '1' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && CPTR_EL3.TTA == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif IsFeatureImplemented(FEAT_TRBE_EXT) && OSLSR_EL1.OSLK == '0' && HaltingAllowed() && EDSCR2.TTA == '1' then Halt(DebugHalt_SoftwareAccess); else TRCCLAIMCLR = X[t, 64]; elsif PSTATE.EL == EL2 then if HaveEL(EL3) && EL3SDDUndefPriority() && CPTR_EL3.TTA == '1' then UNDEFINED; elsif CPTR_EL2.TTA == '1' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && CPTR_EL3.TTA == '1' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif !ELUsingAArch32(EL1) && IsFeatureImplemented(FEAT_TRBE_EXT) && OSLSR_EL1.OSLK == '0' && HaltingAllowed() && EDSCR2.TTA == '1' then Halt(DebugHalt_SoftwareAccess); else TRCCLAIMCLR = X[t, 64]; elsif PSTATE.EL == EL3 then if CPTR_EL3.TTA == '1' then AArch64.SystemAccessTrap(EL3, 0x18); elsif !ELUsingAArch32(EL1) && IsFeatureImplemented(FEAT_TRBE_EXT) && OSLSR_EL1.OSLK == '0' && HaltingAllowed() && EDSCR2.TTA == '1' then Halt(DebugHalt_SoftwareAccess); else TRCCLAIMCLR = X[t, 64];

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.