AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# CNTHVS_CTL, Counter-timer Secure Virtual Timer Control Register (EL2)

The CNTHVS_CTL characteristics are:

## Purpose

Provides AArch32 access from EL0 to the Secure EL2 virtual timer.

## Configuration

AArch32 System register CNTHVS_CTL bits [31:0] are architecturally mapped to AArch64 System register CNTHVS_CTL_EL2[31:0].

This register is present only when AArch32 is supported and FEAT_SEL2 is implemented. Otherwise, direct accesses to CNTHVS_CTL are UNDEFINED.

## Attributes

CNTHVS_CTL is a 32-bit register.

## Field descriptions

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
RES0 | ISTATUS | IMASK | ENABLE

#### Bits [31:3]

Reserved, RES0.

#### ISTATUS, bit [2]

The status of the timer. This bit indicates whether the timer condition is met:

ISTATUS | Meaning
--- | ---
0b0 | Timer condition is not met.
0b1 | Timer condition is met.

When the value of the ENABLE bit is 1, ISTATUS indicates whether the timer condition is met. ISTATUS takes no account of the value of the IMASK bit. If the value of ISTATUS is 1 and the value of IMASK is 0 then the timer interrupt is asserted.

When the value of the ENABLE bit is 0, the ISTATUS field is UNKNOWN.

The reset behavior of this field is:

- On a Warm reset, this field resets to an architecturally UNKNOWN value.

Access to this field is RO.

#### IMASK, bit [1]

Timer interrupt mask bit. Permitted values are:

IMASK | Meaning
--- | ---
0b0 | Timer interrupt is not masked by the IMASK bit.
0b1 | Timer interrupt is masked by the IMASK bit.

For more information, see the description of the ISTATUS bit.

The reset behavior of this field is:

- On a Warm reset, this field resets to an architecturally UNKNOWN value.

#### ENABLE, bit [0]

Enables the timer. Permitted values are:

ENABLE | Meaning
--- | ---
0b0 | Timer disabled.
0b1 | Timer enabled.

Setting this bit to 0 disables the timer output signal, but the timer value accessible from CNTHVS_TVAL continues to count down.

Note

Disabling the output signal might be a power-saving option.

The reset behavior of this field is:

- On a Warm reset, this field resets to an architecturally UNKNOWN value.

## Accessing CNTHVS_CTL

This register is accessed using the encoding for CNTV_CTL.

Accesses to this register use the following encodings in the System register encoding space:

#### MRC{<c>}{<q>} <coproc>, {#}<opc1>, <Rt>, <CRn>, <CRm>{, {#}<opc2>}

coproc | opc1 | CRn | CRm | opc2
--- | --- | --- | --- | ---
0b1111 | 0b000 | 0b1110 | 0b0011 | 0b001

if PSTATE.EL == EL0 then if !ELUsingAArch32(EL1) && !ELIsInHost(EL0) && CNTKCTL_EL1.EL0VTEN == '0' then if EL2Enabled() && !ELUsingAArch32(EL2) && HCR_EL2.TGE == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); else AArch64.AArch32SystemAccessTrap(EL1, 0x03); elsif ELUsingAArch32(EL1) && CNTKCTL.PL0VTEN == '0' then if EL2Enabled() && !ELUsingAArch32(EL2) && HCR_EL2.TGE == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HCR.TGE == '1' then AArch32.TakeHypTrapException(0x00); else UNDEFINED; elsif ELIsInHost(EL0) && CNTHCTL_EL2.EL0VTEN == '0' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && !ELUsingAArch32(EL2) && !ELIsInHost(EL0) && IsFeatureImplemented(FEAT_ECV) && CNTHCTL_EL2.EL1TVT == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif ELIsInHost(EL0) && IsCurrentSecurityState(SS_Secure) && IsFeatureImplemented(FEAT_SEL2) then R[t] = CNTHVS_CTL_EL2<31:0>; elsif ELIsInHost(EL0) && !IsCurrentSecurityState(SS_Secure) then R[t] = CNTHV_CTL_EL2<31:0>; else R[t] = CNTV_CTL; elsif PSTATE.EL == EL1 then if EL2Enabled() && !ELUsingAArch32(EL2) && IsFeatureImplemented(FEAT_ECV) && CNTHCTL_EL2.EL1TVT == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); else R[t] = CNTV_CTL; elsif PSTATE.EL == EL2 then R[t] = CNTV_CTL; elsif PSTATE.EL == EL3 then R[t] = CNTV_CTL;

#### MCR{<c>}{<q>} <coproc>, {#}<opc1>, <Rt>, <CRn>, <CRm>{, {#}<opc2>}

coproc | opc1 | CRn | CRm | opc2
--- | --- | --- | --- | ---
0b1111 | 0b000 | 0b1110 | 0b0011 | 0b001

if PSTATE.EL == EL0 then if !ELUsingAArch32(EL1) && !ELIsInHost(EL0) && CNTKCTL_EL1.EL0VTEN == '0' then if EL2Enabled() && !ELUsingAArch32(EL2) && HCR_EL2.TGE == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); else AArch64.AArch32SystemAccessTrap(EL1, 0x03); elsif ELUsingAArch32(EL1) && CNTKCTL.PL0VTEN == '0' then if EL2Enabled() && !ELUsingAArch32(EL2) && HCR_EL2.TGE == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HCR.TGE == '1' then AArch32.TakeHypTrapException(0x00); else UNDEFINED; elsif ELIsInHost(EL0) && CNTHCTL_EL2.EL0VTEN == '0' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && !ELUsingAArch32(EL2) && !ELIsInHost(EL0) && IsFeatureImplemented(FEAT_ECV) && CNTHCTL_EL2.EL1TVT == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif ELIsInHost(EL0) && IsCurrentSecurityState(SS_Secure) && IsFeatureImplemented(FEAT_SEL2) then CNTHVS_CTL_EL2 = R[t]; elsif ELIsInHost(EL0) && !IsCurrentSecurityState(SS_Secure) then CNTHV_CTL_EL2 = R[t]; else CNTV_CTL = R[t]; elsif PSTATE.EL == EL1 then if EL2Enabled() && !ELUsingAArch32(EL2) && IsFeatureImplemented(FEAT_ECV) && CNTHCTL_EL2.EL1TVT == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); else CNTV_CTL = R[t]; elsif PSTATE.EL == EL2 then CNTV_CTL = R[t]; elsif PSTATE.EL == EL3 then CNTV_CTL = R[t];

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.