AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# PMSDSFR_EL1, Sampling Data Source Filter Register

The PMSDSFR_EL1 characteristics are:

## Purpose

Controls sample filtering by Data Source.

## Configuration

This register is present only when FEAT_SPE_FDS is implemented. Otherwise, direct accesses to PMSDSFR_EL1 are UNDEFINED.

## Attributes

PMSDSFR_EL1 is a 64-bit register.

## Field descriptions

63 | 62 | 61 | 60 | 59 | 58 | 57 | 56 | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48 | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40 | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
S63 | S62 | S61 | S60 | S59 | S58 | S57 | S56 | S55 | S54 | S53 | S52 | S51 | S50 | S49 | S48 | S47 | S46 | S45 | S44 | S43 | S42 | S41 | S40 | S39 | S38 | S37 | S36 | S35 | S34 | S33 | S32
S31 | S30 | S29 | S28 | S27 | S26 | S25 | S24 | S23 | S22 | S21 | S20 | S19 | S18 | S17 | S16 | S15 | S14 | S13 | S12 | S11 | S10 | S9 | S8 | S7 | S6 | S5 | S4 | S3 | S2 | S1 | S0

#### S<m>, bit [m], for m = 63 to 0
When filtering on Data Source <m> is supported:

S[<m>] is the Data Source filter for IMPLEMENTATION DEFINED Data Source <m>.

S<m> | Meaning
--- | ---
0b0 | If PMSFCR_EL1.FDS is 1, do not record load operations that have bits [5:0] of the Data Source packet set to <m>.
0b1 | Load operations with Data Source <m> are unaffected by PMSFCR_EL1.FDS.

The reset behavior of this field is:

- On a Warm reset, this field resets to an architecturally UNKNOWN value.

####
Otherwise:

Reserved, RAZ/WI.

## Accessing PMSDSFR_EL1

Accesses to this register use the following encodings in the System register encoding space:

#### MRS <Xt>, PMSDSFR_EL1

op0 | op1 | CRn | CRm | op2
--- | --- | --- | --- | ---
0b11 | 0b000 | 0b1001 | 0b1010 | 0b100

if PSTATE.EL == EL0 then UNDEFINED; elsif PSTATE.EL == EL1 then if HaveEL(EL3) && EL3SDDUndefPriority() && MDCR_EL3.EnPMS3 == '0' then UNDEFINED; elsif HaveEL(EL3) && EL3SDDUndefPriority() && (MDCR_EL3.NSPB[0] == '0' || MDCR_EL3.NSPB[1] != SCR_EL3.NS || (IsFeatureImplemented(FEAT_RME) && MDCR_EL3.NSPBE != SCR_EL3.NSE)) then UNDEFINED; elsif EL2Enabled() && IsFeatureImplemented(FEAT_FGT2) && ((HaveEL(EL3) && SCR_EL3.FGTEn2 == '0') || HDFGRTR2_EL2.nPMSDSFR_EL1 == '0') then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && MDCR_EL2.TPMS == '1' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && MDCR_EL3.EnPMS3 == '0' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif HaveEL(EL3) && (MDCR_EL3.NSPB[0] == '0' || MDCR_EL3.NSPB[1] != SCR_EL3.NS || (IsFeatureImplemented(FEAT_RME) && MDCR_EL3.NSPBE != SCR_EL3.NSE)) then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif EffectiveHCR_EL2_NVx() IN {'1x1'} then X[t, 64] = NVMem[0x858]; else X[t, 64] = PMSDSFR_EL1; elsif PSTATE.EL == EL2 then if HaveEL(EL3) && EL3SDDUndefPriority() && (MDCR_EL3.NSPB[0] == '0' || MDCR_EL3.NSPB[1] != SCR_EL3.NS || (IsFeatureImplemented(FEAT_RME) && MDCR_EL3.NSPBE != SCR_EL3.NSE)) then UNDEFINED; elsif HaveEL(EL3) && EL3SDDUndefPriority() && MDCR_EL3.EnPMS3 == '0' then UNDEFINED; elsif HaveEL(EL3) && (MDCR_EL3.NSPB[0] == '0' || MDCR_EL3.NSPB[1] != SCR_EL3.NS || (IsFeatureImplemented(FEAT_RME) && MDCR_EL3.NSPBE != SCR_EL3.NSE)) then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif HaveEL(EL3) && MDCR_EL3.EnPMS3 == '0' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); else X[t, 64] = PMSDSFR_EL1; elsif PSTATE.EL == EL3 then X[t, 64] = PMSDSFR_EL1;

#### MSR PMSDSFR_EL1, <Xt>

op0 | op1 | CRn | CRm | op2
--- | --- | --- | --- | ---
0b11 | 0b000 | 0b1001 | 0b1010 | 0b100

if PSTATE.EL == EL0 then UNDEFINED; elsif PSTATE.EL == EL1 then if HaveEL(EL3) && EL3SDDUndefPriority() && MDCR_EL3.EnPMS3 == '0' then UNDEFINED; elsif HaveEL(EL3) && EL3SDDUndefPriority() && (MDCR_EL3.NSPB[0] == '0' || MDCR_EL3.NSPB[1] != SCR_EL3.NS || (IsFeatureImplemented(FEAT_RME) && MDCR_EL3.NSPBE != SCR_EL3.NSE)) then UNDEFINED; elsif EL2Enabled() && IsFeatureImplemented(FEAT_FGT2) && ((HaveEL(EL3) && SCR_EL3.FGTEn2 == '0') || HDFGWTR2_EL2.nPMSDSFR_EL1 == '0') then AArch64.SystemAccessTrap(EL2, 0x18); elsif EL2Enabled() && MDCR_EL2.TPMS == '1' then AArch64.SystemAccessTrap(EL2, 0x18); elsif HaveEL(EL3) && MDCR_EL3.EnPMS3 == '0' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif HaveEL(EL3) && (MDCR_EL3.NSPB[0] == '0' || MDCR_EL3.NSPB[1] != SCR_EL3.NS || (IsFeatureImplemented(FEAT_RME) && MDCR_EL3.NSPBE != SCR_EL3.NSE)) then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif EffectiveHCR_EL2_NVx() IN {'1x1'} then NVMem[0x858] = X[t, 64]; else PMSDSFR_EL1 = X[t, 64]; elsif PSTATE.EL == EL2 then if HaveEL(EL3) && EL3SDDUndefPriority() && (MDCR_EL3.NSPB[0] == '0' || MDCR_EL3.NSPB[1] != SCR_EL3.NS || (IsFeatureImplemented(FEAT_RME) && MDCR_EL3.NSPBE != SCR_EL3.NSE)) then UNDEFINED; elsif HaveEL(EL3) && EL3SDDUndefPriority() && MDCR_EL3.EnPMS3 == '0' then UNDEFINED; elsif HaveEL(EL3) && (MDCR_EL3.NSPB[0] == '0' || MDCR_EL3.NSPB[1] != SCR_EL3.NS || (IsFeatureImplemented(FEAT_RME) && MDCR_EL3.NSPBE != SCR_EL3.NSE)) then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); elsif HaveEL(EL3) && MDCR_EL3.EnPMS3 == '0' then if EL3SDDUndef() then UNDEFINED; else AArch64.SystemAccessTrap(EL3, 0x18); else PMSDSFR_EL1 = X[t, 64]; elsif PSTATE.EL == EL3 then PMSDSFR_EL1 = X[t, 64];

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.