AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# TLBTR, TLB Type Register

The TLBTR characteristics are:

## Purpose

Provides information about the TLB implementation. The register must define whether the implementation provides separate instruction and data TLBs, or a unified TLB. Normally, the IMPLEMENTATION DEFINED information in this register includes the number of lockable entries in the TLB.

## Configuration

This register is present only when EL1 is capable of using AArch32. Otherwise, direct accesses to TLBTR are UNDEFINED.

## Attributes

TLBTR is a 32-bit register.

## Field descriptions

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
IMPLEMENTATION DEFINED | nU

#### IMPLEMENTATION DEFINED, bits [31:1]

IMPLEMENTATION DEFINED.

#### nU, bit [0]

Not Unified TLB. Indicates whether the implementation has a unified TLB.

The value of this field is an IMPLEMENTATION DEFINED choice of:

nU | Meaning
--- | ---
0b0 | Unified TLB.
0b1 | Separate Instruction and Data TLBs.

Access to this field is RO.

## Accessing TLBTR

Accesses to this register use the following encodings in the System register encoding space:

#### MRC{<c>}{<q>} <coproc>, {#}<opc1>, <Rt>, <CRn>, <CRm>{, {#}<opc2>}

coproc | opc1 | CRn | CRm | opc2
--- | --- | --- | --- | ---
0b1111 | 0b000 | 0b0000 | 0b0000 | 0b011

if PSTATE.EL == EL0 then UNDEFINED; elsif PSTATE.EL == EL1 then if EL2Enabled() && !ELUsingAArch32(EL2) && HSTR_EL2.T0 == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HSTR.T0 == '1' then AArch32.TakeHypTrapException(0x03); elsif EL2Enabled() && !ELUsingAArch32(EL2) && HCR_EL2.TID1 == '1' then AArch64.AArch32SystemAccessTrap(EL2, 0x03); elsif EL2Enabled() && ELUsingAArch32(EL2) && HCR.TID1 == '1' then AArch32.TakeHypTrapException(0x03); else R[t] = TLBTR; elsif PSTATE.EL == EL2 then R[t] = TLBTR; elsif PSTATE.EL == EL3 then R[t] = TLBTR;

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.