Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## ADC

Add with Carry adds two register values and the Carry flag value, and writes the result to the destination register.

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
sf | 0 | 0 | 1 | 1 | 0 | 1 | 0 | 0 | 0 | 0 | Rm | 0 | 0 | 0 | 0 | 0 | 0 | Rn | Rd
| op | S |  |  |  |  |

#### 32-bit (sf == 0)

ADC <Wd>, <Wn>, <Wm>

#### 64-bit (sf == 1)

ADC <Xd>, <Xn>, <Xm>

integer d = UInt(Rd); integer n = UInt(Rn); integer m = UInt(Rm); constant integer datasize = 32 << UInt(sf);

### Assembler Symbols

<Wd> | Is the 32-bit name of the general-purpose destination register, encoded in the "Rd" field.

<Wn> | Is the 32-bit name of the first general-purpose source register, encoded in the "Rn" field.

<Wm> | Is the 32-bit name of the second general-purpose source register, encoded in the "Rm" field.

<Xd> | Is the 64-bit name of the general-purpose destination register, encoded in the "Rd" field.

<Xn> | Is the 64-bit name of the first general-purpose source register, encoded in the "Rn" field.

<Xm> | Is the 64-bit name of the second general-purpose source register, encoded in the "Rm" field.

### Operation

bits(datasize) result; bits(datasize) operand1 = X[n, datasize]; bits(datasize) operand2 = X[m, datasize]; (result, -) = AddWithCarry(operand1, operand2, PSTATE.C); X[d, datasize] = result;

### Operational information

If PSTATE.DIT is 1:

- The execution time of this instruction is independent of:
  - The values of the data supplied in any of its registers.
  - The values of the NZCV flags.
- The response of this instruction to asynchronous exceptions does not vary based on:
  - The values of the data supplied in any of its registers.
  - The values of the NZCV flags.

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: isa v33.74, AdvSIMD v29.23, pseudocode v2023-09_rel, sve v2023-09_rc3 ; Build timestamp: 2023-09-27T17:06

Copyright © 2010-2023 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.