Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## LASTB (SIMD&FP scalar)

Extract last element to SIMD&FP scalar register

If there is an active element then extract the last active element from the final source vector register. If there are no active elements, extract the highest-numbered element. Then place the extracted element in the destination SIMD&FP register.

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | 0 | 0 | 0 | 0 | 1 | 0 | 1 | size | 1 | 0 | 0 | 0 | 1 | 1 | 1 | 0 | 0 | Pg | Zn | Vd
|  |  | B |  |  |  |

####

LASTB <V><d>, <Pg>, <Zn>.<T>

if !IsFeatureImplemented(FEAT_SVE) && !IsFeatureImplemented(FEAT_SME) then UNDEFINED; constant integer esize = 8 << UInt(size); constant integer g = UInt(Pg); constant integer n = UInt(Zn); constant integer d = UInt(Vd); constant boolean isBefore = TRUE;

### Assembler Symbols

<V> | Is a width specifier, encoded in size:
size | <V>
--- | ---
00 | B
01 | H
10 | S
11 | D

<d> | Is the number [0-31] of the destination SIMD&FP register, encoded in the "Vd" field.

<Pg> | Is the name of the governing scalable predicate register P0-P7, encoded in the "Pg" field.

<Zn> | Is the name of the source scalable vector register, encoded in the "Zn" field.

<T> | Is the size specifier, encoded in size:
size | <T>
--- | ---
00 | B
01 | H
10 | S
11 | D

### Operation

CheckSVEEnabled(); constant integer VL = CurrentVL; constant integer PL = VL DIV 8; constant integer elements = VL DIV esize; constant bits(PL) mask = P[g, PL]; constant bits(VL) operand = Z[n, VL]; integer last = LastActiveElement(mask, esize); if isBefore then if last < 0 then last = elements - 1; else last = last + 1; if last >= elements then last = 0; V[d, esize] = Elem[operand, last, esize];

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: aarchmrs v2024-03_relA, pseudocode v2024-03_rel, sve v2024-03_rel ; Build timestamp: 2024-03-26T09:45

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.