Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## SQXTUNT

Signed saturating unsigned extract narrow (top)

Saturate the signed integer value in each source element to an unsigned integer value that is half the original source element width, and place the results in the odd-numbered half-width destination elements, leaving the even-numbered elements unchanged.

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | 1 | 0 | 0 | 0 | 1 | 0 | 1 | 0 | tszh | 1 | tszl | 0 | 0 | 0 | 0 | 1 | 0 | 1 | 0 | 1 | Zn | Zd
|  |  |  |  |  |  | T |  |

####

SQXTUNT <Zd>.<T>, <Zn>.<Tb>

if !IsFeatureImplemented(FEAT_SVE2) && !IsFeatureImplemented(FEAT_SME) then UNDEFINED; constant bits(3) tsize = tszh:tszl; integer esize; case tsize of when '001' esize = 16; when '010' esize = 32; when '100' esize = 64; otherwise UNDEFINED; constant integer n = UInt(Zn); constant integer d = UInt(Zd);

### Assembler Symbols

<Zd> | Is the name of the destination scalable vector register, encoded in the "Zd" field.

<T> | Is the size specifier, encoded in tszh:tszl:
tszh | tszl | <T>
--- | --- | ---
0 | 00 | RESERVED
0 | 01 | B
0 | 10 | H
x | 11 | RESERVED
1 | 00 | S
1 | 01 | RESERVED
1 | 10 | RESERVED

<Zn> | Is the name of the source scalable vector register, encoded in the "Zn" field.

<Tb> | Is the size specifier, encoded in tszh:tszl:
tszh | tszl | <Tb>
--- | --- | ---
0 | 00 | RESERVED
0 | 01 | H
0 | 10 | S
x | 11 | RESERVED
1 | 00 | D
1 | 01 | RESERVED
1 | 10 | RESERVED

### Operation

CheckSVEEnabled(); constant integer VL = CurrentVL; constant integer PL = VL DIV 8; constant integer elements = VL DIV esize; constant bits(VL) operand1 = Z[n, VL]; bits(VL) result = Z[d, VL]; constant integer halfesize = esize DIV 2; for e = 0 to elements-1 constant integer element1 = SInt(Elem[operand1, e, esize]); constant bits(halfesize) res = UnsignedSat(element1, halfesize); Elem[result, 2*e + 1, halfesize] = res; Z[d, VL] = result;

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: aarchmrs v2024-03_relA, pseudocode v2024-03_rel, sve v2024-03_rel ; Build timestamp: 2024-03-26T09:45

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.