AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# RVBAR_EL1, Reset Vector Base Address Register (if EL2 and EL3 not implemented)

The RVBAR_EL1 characteristics are:

## Purpose

If EL1 is the highest Exception level implemented, contains the IMPLEMENTATION DEFINED address that execution starts from after reset when executing in AArch64 state.

## Configuration

This register is present only when the highest implemented Exception level is EL1. Otherwise, direct accesses to RVBAR_EL1 are UNDEFINED.

## Attributes

RVBAR_EL1 is a 64-bit register.

## Field descriptions

63 | 62 | 61 | 60 | 59 | 58 | 57 | 56 | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48 | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40 | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
ResetAddress
ResetAddress

#### ResetAddress, bits [63:0]

The IMPLEMENTATION DEFINED address that execution starts from after reset when executing in 64-bit state. Bits[1:0] of this register are 00, as this address must be aligned, and the address must be within the physical address size supported by the PE.

This field has an IMPLEMENTATION DEFINED value.

Access to this field is RO.

## Accessing RVBAR_EL1

Accesses to this register use the following encodings in the System register encoding space:

#### MRS <Xt>, RVBAR_EL1

op0 | op1 | CRn | CRm | op2
--- | --- | --- | --- | ---
0b11 | 0b000 | 0b1100 | 0b0000 | 0b001

if PSTATE.EL == EL1 && IsHighestEL(EL1) then X[t, 64] = RVBAR_EL1; else UNDEFINED;

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.