AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# ERR<n>PFGCDN, Error Record <n> Pseudo-fault Generation Countdown Register, n = 0 - 65534

The ERR<n>PFGCDN characteristics are:

## Purpose

Generates one of the errors enabled in the corresponding ERR<n>PFGCTL register.

## Configuration

This register is present only when error record n is implemented, the node that owns error record n implements the Common Fault Injection Model Extension and error record n is the first error record in the node. Otherwise, direct accesses to ERR<n>PFGCDN are RES0.

ERR<n>FR describes the features implemented by the node.

## Attributes

ERR<n>PFGCDN is a 64-bit register.

## Field descriptions

63 | 62 | 61 | 60 | 59 | 58 | 57 | 56 | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48 | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40 | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
RES0
CDN

#### Bits [63:32]

Reserved, RES0.

#### CDN, bits [31:0]

Countdown value.

This field is copied to Error Generation Counter when either:

- Software writes 1 to ERR<n>PFGCTL.CDNEN.
- The Error Generation Counter decrements to zero and ERR<n>PFGCTL.R is 1.

While ERR<n>PFGCTL.CDNEN is 1 and the Error Generation Counter is nonzero, the counter decrements by 1 for each cycle at an IMPLEMENTATION DEFINED clock rate. When the counter reaches zero, one of the errors enabled in the ERR<n>PFGCTL register is generated.

Note

The current Error Generation Counter value is not visible to software.

The reset behavior of this field is:

- On a Cold reset, this field resets to an architecturally UNKNOWN value.

## Accessing ERR<n>PFGCDN

#### ERR<n>PFGCDN can be accessed through the memory-mapped interfaces:

Component | Offset | Instance
--- | --- | ---
RAS | 0x810 + (64 * n) | ERR<n>PFGCDN

Accesses on this interface are RW.

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.