Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## REV (vector)

Reverse all elements in a vector (unpredicated)

Reverse the order of all elements in the source vector and place in the destination vector. This instruction is unpredicated.

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | 0 | 0 | 0 | 0 | 1 | 0 | 1 | size | 1 | 1 | 1 | 0 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 0 | Zn | Zd

####

REV <Zd>.<T>, <Zn>.<T>

if !HaveSVE() && !HaveSME() then UNDEFINED; constant integer esize = 8 << UInt(size); integer n = UInt(Zn); integer d = UInt(Zd);

### Assembler Symbols

<Zd> | Is the name of the destination scalable vector register, encoded in the "Zd" field.

<T> | Is the size specifier, encoded in size:
size | <T>
--- | ---
00 | B
01 | H
10 | S
11 | D

<Zn> | Is the name of the source scalable vector register, encoded in the "Zn" field.

### Operation

CheckSVEEnabled(); constant integer VL = CurrentVL; constant integer PL = VL DIV 8; bits(VL) operand = Z[n, VL]; bits(VL) result = Reverse(operand, esize); Z[d, VL] = result;

### Operational information

If FEAT_SVE2 is implemented or FEAT_SME is implemented, then if PSTATE.DIT is 1:

- The execution time of this instruction is independent of:
  - The values of the data supplied in any of its registers.
  - The values of the NZCV flags.
- The response of this instruction to asynchronous exceptions does not vary based on:
  - The values of the data supplied in any of its registers.
  - The values of the NZCV flags.

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: isa v33.74, AdvSIMD v29.23, pseudocode v2023-09_rel, sve v2023-09_rc3 ; Build timestamp: 2023-09-27T17:06

Copyright © 2010-2023 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.