Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

## MVN

Bitwise NOT (vector). This instruction reads each vector element from the source SIMD&FP register, places the inverse of each value into a vector, and writes the vector to the destination SIMD&FP register.

Depending on the settings in the CPACR_EL1, CPTR_EL2, and CPTR_EL3 registers, and the current Security state and Exception level, an attempt to execute the instruction might be trapped.

This is an alias of NOT. This means:

- The encodings in this description are named to match the encodings of NOT.
- The description of NOT gives the operational pseudocode, any constrained unpredictable behavior, and any operational information for this instruction.

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
0 | Q | 1 | 0 | 1 | 1 | 1 | 0 | 0 | 0 | 1 | 0 | 0 | 0 | 0 | 0 | 0 | 1 | 0 | 1 | 1 | 0 | Rn | Rd

####

MVN <Vd>.<T>, <Vn>.<T>

is equivalent to

NOT <Vd>.<T>, <Vn>.<T>

and is always the preferred disassembly.

### Assembler Symbols

<Vd> | Is the name of the SIMD&FP destination register, encoded in the "Rd" field.

<T> | Is an arrangement specifier, encoded in Q:
Q | <T>
--- | ---
0 | 8B
1 | 16B

<Vn> | Is the name of the SIMD&FP source register, encoded in the "Rn" field.

### Operation

The description of NOT gives the operational pseudocode for this instruction.

### Operational information

If PSTATE.DIT is 1:

- The execution time of this instruction is independent of:
  - The values of the data supplied in any of its registers.
  - The values of the NZCV flags.
- The response of this instruction to asynchronous exceptions does not vary based on:
  - The values of the data supplied in any of its registers.
  - The values of the NZCV flags.

Base Instructions | SIMD&FP Instructions | SVE Instructions | SME Instructions | Index by Encoding | Shared Pseudocode | Proprietary Notice

Internal version only: isa v33.64, AdvSIMD v29.12, pseudocode v2023-06_rel, sve v2023-06_rel ; Build timestamp: 2023-07-04T19:42

Copyright © 2010-2023 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.