AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

# TRCIDR9, Trace ID Register 9

The TRCIDR9 characteristics are:

## Purpose

Returns the tracing capabilities of the trace unit.

## Configuration

External register TRCIDR9 bits [31:0] are architecturally mapped to AArch64 System register TRCIDR9[31:0].

This register is present only when FEAT_ETE is implemented and FEAT_TRC_EXT is implemented. Otherwise, direct accesses to TRCIDR9 are RES0.

## Attributes

TRCIDR9 is a 32-bit register.

## Field descriptions

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
NUMP0KEY

#### NUMP0KEY, bits [31:0]
When TRCIDR0.TRCDATA != 0b00:

Indicates the number of P0 right-hand keys. Data tracing is not implemented in ETE and this field is reserved for other trace architectures. Allocated in other trace architectures.

This field has an IMPLEMENTATION DEFINED value.

Access to this field is RO.

####
Otherwise:

Reserved, RES0.

## Accessing TRCIDR9

#### TRCIDR9 can be accessed through the external debug interface:

Component | Offset | Instance
--- | --- | ---
ETE | 0x184 | TRCIDR9

This interface is accessible as follows:

- When OSLockStatus() or !IsTraceCorePowered(), accesses to this register generate an error response.
- Otherwise, accesses to this register are RO.

AArch32 Registers | AArch64 Registers | AArch32 Instructions | AArch64 Instructions | Index by Encoding | External Registers | External Registers by Offset | Registers by Functional Group | Proprietary Notice

26/03/2024 09:49; 67c0ae5282a7629ba0ea0ba7267b43cd4f7939f6

Copyright © 2010-2024 Arm Limited or its affiliates. All rights reserved. This document is Non-Confidential.